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Description automatically generated]	AUV Post Dive Report	AUV Operations


	Date:
	22-23Sep 2020

	Vehicle:
	I2Map

	Location:
	36.6969, -122.0470

	Major Objective:
	Overnight Transect Mission

	Dive Plan:
	Deimos_Transect_202000922.cfg



Accomplishments:

· Vehicle started night dive set at 22:55L (22:30L was desired night transect timeout).
· No timeouts or spurious log entries from CARL Server.
· No CTD dropouts, and PAR data contained fully in seabird25p.log

Vehicle Issues:
· Required second mission launch, as exception was thrown from DVL driver, with the following syslog error, 

“: dvl - caught Exception: Buffer Full”

Note(s):
· Vehicle was rinsed and main batteries charged while on deck.
· Oil comp was empty on recovery.
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