
[image: ]	AUV Post Dive Report	AUV Operations


	Date:
	3/31/2021

	Vehicle:
	I2MAP

	Location:
	M1

	Major Objective:
	     

	Dive Plan:
	[bookmark: Text4]     



AUV Operators:
Launch: Erik Trauschke, Chris Wahl, Emery Nolasco
Recovery: Chris Wahl, Emery Nolasco

Accomplishments:
The vehicle was deployed, recovered, and performed as programmed. 
[bookmark: _GoBack]
Vehicle Issues:
The vehicle operated as scripted. It moved slower than usual which may have contributed to the longer transect times. 
-We need a way to communicate with the vehicle underwater and have the ability to kill a mission. 
-Check the status of the dropweight. We had intermittent connection with the vehicle once it reached the surface and we weren’t able to recover the vehicle until about 12:30 after the vehicle had surface around 10:30.

Note(s):
-Creating a way to visualize the script to double check the timing and planned mission before executing would help catch mistakes
-The time relative execution can cause error stack ups, if there is a way to make the events actual time triggered instead of relative it may make the mission more accurate
-Thought: Would it be possible and/or useful to have the waveglider provide data to the vehicle for location precision?
-   Planned on vehicle to come up at 8am. When we approached the station, at 8:30 with the poles down, the vehicle had just started it’s last series of transects for 600 to 1000m. With no way to kill the mission we had to wait until the vehicle was done with it’s mission or timed out.
-Could we make a script that turns off all the batteries?
-Check vehicle pitch from previous missions to see if the movement of the weight bags from fwd to aft helped the pitch angle.
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