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	Date:
	July 7 2020

	Vehicle:
	Mapper 1

	Location:
	Head of Monterey Canyon (36.778781 -121.872006)

	Major Objective:
	Patch test of multibeam sonar

	Dive Plan:
	Deploy, run 20190308_PatchTest_1v1.cfg, recover



Accomplishments:
Ran two missions on Mapper 1. First was with sonar in CW mode, second in FM. Used automatic tracker for setting pulse width. We didn’t configure the tracker to control power or gain, we aren’t sure if this will turn the power up while on deck





Vehicle Issues:
[bookmark: _GoBack]Possible PPS timing issue with Mapper 1 T50. BITE indicates that PPS isn’t being detected by sonar hardware (DMPA board), although it is being detected by serial port hardware handshake line. Possible wiring or signal level problem. No other issues noted.





Note(s):
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