MBARI AUV Operations Service ARGOS

I purchased a Telonics ST-20 Model A-1010 self contained battery powered location only transmitter.  The serial number is 519012 PO reference 0311565.  Nominally good to 1000 m, this unit is meant to serve the extended AUV CTD project missions as a backup emergency location aid.

From our Service ARGOS use agreement:

Program Number 2726

Name of the Program:  MBARI AUV Operations

Program administrator:  Gashler Drew

Starting Date 01 June 2003

Ending Date 31 May 2006

The access codes to our Argos data:

Username: Gashler

User password: Suroko

Program password: Fuji

PTT Id number

Decimal

42606

Hex


34D2DE1

Repetition period 
90


To access the latest location data:

telnet datadist.argosinc.com

You will see:

Welcome to OpenVMS ™ Alpha Operating System, Version V7.2-1

Username: Gashler

Password:  



Welcome to the North American global processing center.


LOGIN AT 239/1815  LAST ACCESS At 239 1759 UTC

ARGOS READY

/
At the / prompt type COM,,,ALL or to see results from last 9 days, 

At the prompt type PRV,,DS,, 

You will see something like 

Prog 2726

42606
33.385N
111.814W
3
231/1535Z-231-1529

(6)

00



00


ARGOS READY

/
Also, type PRV/A,2726,DS,59,

You wil see something like:

02726 42606   4 31 D 2005-03-02 03:13:23  36.522 -121.671  0.000  401649802
      2005-03-02 15:36:36  1         00           00           00

      2005-03-02 15:38:06  1         00           51           25

      2005-03-02 15:39:36  1         00           00           00

02726 42606   2 31 J

      2005-03-02 15:38:06  4         00           00           00

02726 42606   2 31 K

      2005-03-02 16:26:06  4         00           00           00

02726 42606   2 31 M

      2005-03-02 16:47:06  1         00           00           00

02726 42606   2 31 J

      2005-03-02 17:21:36  7         00           00           00

There is a charge based upon time connected, so when you are done:

ARGOS READY

/LOGOUT
For more command information refer to section 4.4 of:

http://www.cls.fr/manuel/
For satellite pass prediction:

http://liftoff.msfc.nasa.gov/RealTime/JPass/20/
NOAA 15 and NOAA 16 are the current operational satellites.



