Data Structures | Defines | Typedefs | Enumerations | Functions

# arm_math.h File Reference

`#include "ARMCM4.h"`
`#include "string.h"`
`#include "math.h"`

Go to the source code of this file.

## Data Structures
struct | arm_fir_instance_q7
| Instance structure for the Q7 FIR filter. More...
struct | arm_fir_instance_q15
| Instance structure for the Q15 FIR filter. More...
struct | arm_fir_instance_q31
| Instance structure for the Q31 FIR filter. More...
struct | arm_fir_instance_f32
| Instance structure for the floating-point FIR filter. More...
struct | arm_biquad_casd_df1_inst_q15
| Instance structure for the Q15 Biquad cascade filter. More...
struct | arm_biquad_casd_df1_inst_q31
| Instance structure for the Q31 Biquad cascade filter. More...
struct | arm_biquad_casd_df1_inst_f32
| Instance structure for the floating-point Biquad cascade filter. More...
struct | arm_matrix_instance_f32
| Instance structure for the floating-point matrix structure. More...
struct | arm_matrix_instance_q15
| Instance structure for the Q15 matrix structure. More...
struct | arm_matrix_instance_q31
| Instance structure for the Q31 matrix structure. More...
struct | arm_pid_instance_q15
| Instance structure for the Q15 PID Control. More...
struct | arm_pid_instance_q31
| Instance structure for the Q31 PID Control. More...
struct | arm_pid_instance_f32
| Instance structure for the floating-point PID Control. More...
struct | arm_linear_interp_instance_f32
| Instance structure for the floating-point Linear Interpolate function. More...
struct | arm_bilinear_interp_instance_f32
| Instance structure for the floating-point bilinear interpolation function. More...
struct | arm_bilinear_interp_instance_q31
| Instance structure for the Q31 bilinear interpolation function. More...
struct | arm_bilinear_interp_instance_q15
| Instance structure for the Q15 bilinear interpolation function. More...
struct | arm_bilinear_interp_instance_q7
| Instance structure for the Q15 bilinear interpolation function. More...
struct | arm_cfft_radix4_instance_q15
| Instance structure for the Q15 CFFT/CIFFT function. More...
struct | arm_cfft_radix4_instance_q31
| Instance structure for the Q31 CFFT/CIFFT function. More...
struct | arm_cfft_radix4_instance_f32
| Instance structure for the floating-point CFFT/CIFFT function. More...
struct | arm_rfft_instance_q15
| Instance structure for the Q15 RFFT/RIFFT function. More...
struct | arm_rfft_instance_q31
| Instance structure for the Q31 RFFT/RIFFT function. More...
struct | arm_rfft_instance_f32
| Instance structure for the floating-point RFFT/RIFFT function. More...
struct | arm_dct4_instance_f32
| Instance structure for the floating-point DCT4/IDCT4 function. More...
struct | arm_dct4_instance_q31
| Instance structure for the Q31 DCT4/IDCT4 function. More...
struct | arm_dct4_instance_q15
| Instance structure for the Q15 DCT4/IDCT4 function. More...
struct | arm_fir_decimate_instance_q15
| Instance structure for the Q15 FIR decimator. More...
struct | arm_fir_decimate_instance_q31
| Instance structure for the Q31 FIR decimator. More...
struct | arm_fir_decimate_instance_f32
| Instance structure for the floating-point FIR decimator. More...
struct | arm_fir_interpolate_instance_q15
| Instance structure for the Q15 FIR interpolator. More...
struct | arm_fir_interpolate_instance_q31
| Instance structure for the Q31 FIR interpolator. More...
struct | arm_fir_interpolate_instance_f32
| Instance structure for the floating-point FIR interpolator. More...
struct | arm_biquad_cas_df1_32x64_ins_q31
| Instance structure for the high precision Q31 Biquad cascade filter. More...
struct | arm_biquad_cascade_df2T_instance_f32
| Instance structure for the floating-point transposed direct form II Biquad cascade filter. More...
struct | arm_fir_lattice_instance_q15
| Instance structure for the Q15 FIR lattice filter. More...
struct | arm_fir_lattice_instance_q31
| Instance structure for the Q31 FIR lattice filter. More...
struct | arm_fir_lattice_instance_f32
| Instance structure for the floating-point FIR lattice filter. More...
struct | arm_iir_lattice_instance_q15
| Instance structure for the Q15 IIR lattice filter. More...
struct | arm_iir_lattice_instance_q31
| Instance structure for the Q31 IIR lattice filter. More...
struct | arm_iir_lattice_instance_f32
| Instance structure for the floating-point IIR lattice filter. More...
struct | arm_lms_instance_f32
| Instance structure for the floating-point LMS filter. More...
struct | arm_lms_instance_q15
| Instance structure for the Q15 LMS filter. More...
struct | arm_lms_instance_q31
| Instance structure for the Q31 LMS filter. More...
struct | arm_lms_norm_instance_f32
| Instance structure for the floating-point normalized LMS filter. More...
struct | arm_lms_norm_instance_q31
| Instance structure for the Q31 normalized LMS filter. More...
struct | arm_lms_norm_instance_q15
| Instance structure for the Q15 normalized LMS filter. More...
struct | arm_fir_sparse_instance_f32
| Instance structure for the floating-point sparse FIR filter. More...
struct | arm_fir_sparse_instance_q31
| Instance structure for the Q31 sparse FIR filter. More...
struct | arm_fir_sparse_instance_q15
| Instance structure for the Q15 sparse FIR filter. More...
struct | arm_fir_sparse_instance_q7
| Instance structure for the Q7 sparse FIR filter. More...
## Defines
#define | __CMSIS_GENERIC
#define | DELTA_Q31 (0x100)
#define | DELTA_Q15 0x5
#define | INDEX_MASK 0x0000003F
#define | PI 3.14159265358979f
#define | TABLE_SIZE 256
#define | TABLE_SPACING_Q31 0x800000
#define | TABLE_SPACING_Q15 0x80
#define | INPUT_SPACING 0xB60B61
#define | __SIMD32(addr) (*(int32_t **) & (addr))
#define | __PACKq7(v0, v1, v2, v3)
## Typedefs
typedef int8_t | q7_t
typedef int16_t | q15_t
typedef int32_t | q31_t
typedef int64_t | q63_t
typedef float | float32_t
typedef double | float64_t
## Enumerations
enum | arm_status { ARM_MATH_SUCCESS = 0, ARM_MATH_ARGUMENT_ERROR = -1, ARM_MATH_LENGTH_ERROR = -2, ARM_MATH_SIZE_MISMATCH = -3, ARM_MATH_NANINF = -4, ARM_MATH_SINGULAR = -5, ARM_MATH_TEST_FAILURE = -6 }
## Functions
static __INLINE q31_t | clip_q63_to_q31 (q63_t x)
static __INLINE q15_t | clip_q63_to_q15 (q63_t x)
static __INLINE q7_t | clip_q31_to_q7 (q31_t x)
static __INLINE q15_t | clip_q31_to_q15 (q31_t x)
static __INLINE q63_t | mult32x64 (q63_t x, q31_t y)
static __INLINE uint32_t | arm_recip_q31 (q31_t in, q31_t *dst, q31_t *pRecipTable)
static __INLINE uint32_t | arm_recip_q15 (q15_t in, q15_t *dst, q15_t *pRecipTable)
void | arm_fir_q7 (const arm_fir_instance_q7 *S, q7_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_fir_init_q7 (arm_fir_instance_q7 *S, uint16_t numTaps, q7_t *pCoeffs, q7_t *pState, uint32_t blockSize)
void | arm_fir_q15 (const arm_fir_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_fir_fast_q15 (const arm_fir_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
arm_status | arm_fir_init_q15 (arm_fir_instance_q15 *S, uint16_t numTaps, q15_t *pCoeffs, q15_t *pState, uint32_t blockSize)
void | arm_fir_q31 (const arm_fir_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_fir_fast_q31 (const arm_fir_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_fir_init_q31 (arm_fir_instance_q31 *S, uint16_t numTaps, q31_t *pCoeffs, q31_t *pState, uint32_t blockSize)
void | arm_fir_f32 (const arm_fir_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_fir_init_f32 (arm_fir_instance_f32 *S, uint16_t numTaps, float32_t *pCoeffs, float32_t *pState, uint32_t blockSize)
void | arm_biquad_cascade_df1_q15 (const arm_biquad_casd_df1_inst_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df1_init_q15 (arm_biquad_casd_df1_inst_q15 *S, uint8_t numStages, q15_t *pCoeffs, q15_t *pState, int8_t postShift)
void | arm_biquad_cascade_df1_fast_q15 (const arm_biquad_casd_df1_inst_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df1_q31 (const arm_biquad_casd_df1_inst_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df1_fast_q31 (const arm_biquad_casd_df1_inst_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df1_init_q31 (arm_biquad_casd_df1_inst_q31 *S, uint8_t numStages, q31_t *pCoeffs, q31_t *pState, int8_t postShift)
void | arm_biquad_cascade_df1_f32 (const arm_biquad_casd_df1_inst_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df1_init_f32 (arm_biquad_casd_df1_inst_f32 *S, uint8_t numStages, float32_t *pCoeffs, float32_t *pState)
arm_status | arm_mat_add_f32 (const arm_matrix_instance_f32 *pSrcA, const arm_matrix_instance_f32 *pSrcB, arm_matrix_instance_f32 *pDst)
arm_status | arm_mat_add_q15 (const arm_matrix_instance_q15 *pSrcA, const arm_matrix_instance_q15 *pSrcB, arm_matrix_instance_q15 *pDst)
arm_status | arm_mat_add_q31 (const arm_matrix_instance_q31 *pSrcA, const arm_matrix_instance_q31 *pSrcB, arm_matrix_instance_q31 *pDst)
arm_status | arm_mat_trans_f32 (const arm_matrix_instance_f32 *pSrc, arm_matrix_instance_f32 *pDst)
arm_status | arm_mat_trans_q15 (const arm_matrix_instance_q15 *pSrc, arm_matrix_instance_q15 *pDst)
arm_status | arm_mat_trans_q31 (const arm_matrix_instance_q31 *pSrc, arm_matrix_instance_q31 *pDst)
arm_status | arm_mat_mult_f32 (const arm_matrix_instance_f32 *pSrcA, const arm_matrix_instance_f32 *pSrcB, arm_matrix_instance_f32 *pDst)
arm_status | arm_mat_mult_q15 (const arm_matrix_instance_q15 *pSrcA, const arm_matrix_instance_q15 *pSrcB, arm_matrix_instance_q15 *pDst, q15_t *pState)
arm_status | arm_mat_mult_fast_q15 (const arm_matrix_instance_q15 *pSrcA, const arm_matrix_instance_q15 *pSrcB, arm_matrix_instance_q15 *pDst, q15_t *pState)
arm_status | arm_mat_mult_q31 (const arm_matrix_instance_q31 *pSrcA, const arm_matrix_instance_q31 *pSrcB, arm_matrix_instance_q31 *pDst)
arm_status | arm_mat_mult_fast_q31 (const arm_matrix_instance_q31 *pSrcA, const arm_matrix_instance_q31 *pSrcB, arm_matrix_instance_q31 *pDst)
arm_status | arm_mat_sub_f32 (const arm_matrix_instance_f32 *pSrcA, const arm_matrix_instance_f32 *pSrcB, arm_matrix_instance_f32 *pDst)
arm_status | arm_mat_sub_q15 (const arm_matrix_instance_q15 *pSrcA, const arm_matrix_instance_q15 *pSrcB, arm_matrix_instance_q15 *pDst)
arm_status | arm_mat_sub_q31 (const arm_matrix_instance_q31 *pSrcA, const arm_matrix_instance_q31 *pSrcB, arm_matrix_instance_q31 *pDst)
arm_status | arm_mat_scale_f32 (const arm_matrix_instance_f32 *pSrc, float32_t scale, arm_matrix_instance_f32 *pDst)
arm_status | arm_mat_scale_q15 (const arm_matrix_instance_q15 *pSrc, q15_t scaleFract, int32_t shift, arm_matrix_instance_q15 *pDst)
arm_status | arm_mat_scale_q31 (const arm_matrix_instance_q31 *pSrc, q31_t scaleFract, int32_t shift, arm_matrix_instance_q31 *pDst)
void | arm_mat_init_q31 (arm_matrix_instance_q31 *S, uint16_t nRows, uint16_t nColumns, q31_t *pData)
void | arm_mat_init_q15 (arm_matrix_instance_q15 *S, uint16_t nRows, uint16_t nColumns, q15_t *pData)
void | arm_mat_init_f32 (arm_matrix_instance_f32 *S, uint16_t nRows, uint16_t nColumns, float32_t *pData)
void | arm_pid_init_f32 (arm_pid_instance_f32 *S, int32_t resetStateFlag)
void | arm_pid_reset_f32 (arm_pid_instance_f32 *S)
void | arm_pid_init_q31 (arm_pid_instance_q31 *S, int32_t resetStateFlag)
void | arm_pid_reset_q31 (arm_pid_instance_q31 *S)
void | arm_pid_init_q15 (arm_pid_instance_q15 *S, int32_t resetStateFlag)
void | arm_pid_reset_q15 (arm_pid_instance_q15 *S)
void | arm_mult_q7 (q7_t *pSrcA, q7_t *pSrcB, q7_t *pDst, uint32_t blockSize)
void | arm_mult_q15 (q15_t *pSrcA, q15_t *pSrcB, q15_t *pDst, uint32_t blockSize)
void | arm_mult_q31 (q31_t *pSrcA, q31_t *pSrcB, q31_t *pDst, uint32_t blockSize)
void | arm_mult_f32 (float32_t *pSrcA, float32_t *pSrcB, float32_t *pDst, uint32_t blockSize)
void | arm_cfft_radix4_q15 (const arm_cfft_radix4_instance_q15 *S, q15_t *pSrc)
arm_status | arm_cfft_radix4_init_q15 (arm_cfft_radix4_instance_q15 *S, uint16_t fftLen, uint8_t ifftFlag, uint8_t bitReverseFlag)
void | arm_cfft_radix4_q31 (const arm_cfft_radix4_instance_q31 *S, q31_t *pSrc)
arm_status | arm_cfft_radix4_init_q31 (arm_cfft_radix4_instance_q31 *S, uint16_t fftLen, uint8_t ifftFlag, uint8_t bitReverseFlag)
void | arm_cfft_radix4_f32 (const arm_cfft_radix4_instance_f32 *S, float32_t *pSrc)
arm_status | arm_cfft_radix4_init_f32 (arm_cfft_radix4_instance_f32 *S, uint16_t fftLen, uint8_t ifftFlag, uint8_t bitReverseFlag)
void | arm_radix4_butterfly_f32 (float32_t *pSrc, uint16_t fftLen, float32_t *pCoef, uint16_t twidCoefModifier)
void | arm_radix4_butterfly_inverse_f32 (float32_t *pSrc, uint16_t fftLen, float32_t *pCoef, uint16_t twidCoefModifier, float32_t onebyfftLen)
void | arm_bitreversal_f32 (float32_t *pSrc, uint16_t fftSize, uint16_t bitRevFactor, uint16_t *pBitRevTab)
void | arm_radix4_butterfly_q31 (q31_t *pSrc, uint32_t fftLen, q31_t *pCoef, uint32_t twidCoefModifier)
void | arm_radix4_butterfly_inverse_q31 (q31_t *pSrc, uint32_t fftLen, q31_t *pCoef, uint32_t twidCoefModifier)
void | arm_bitreversal_q31 (q31_t *pSrc, uint32_t fftLen, uint16_t bitRevFactor, uint16_t *pBitRevTab)
void | arm_radix4_butterfly_q15 (q15_t *pSrc16, uint32_t fftLen, q15_t *pCoef16, uint32_t twidCoefModifier)
void | arm_radix4_butterfly_inverse_q15 (q15_t *pSrc16, uint32_t fftLen, q15_t *pCoef16, uint32_t twidCoefModifier)
void | arm_bitreversal_q15 (q15_t *pSrc, uint32_t fftLen, uint16_t bitRevFactor, uint16_t *pBitRevTab)
void | arm_rfft_q15 (const arm_rfft_instance_q15 *S, q15_t *pSrc, q15_t *pDst)
arm_status | arm_rfft_init_q15 (arm_rfft_instance_q15 *S, arm_cfft_radix4_instance_q15 *S_CFFT, uint32_t fftLenReal, uint32_t ifftFlagR, uint32_t bitReverseFlag)
void | arm_rfft_q31 (const arm_rfft_instance_q31 *S, q31_t *pSrc, q31_t *pDst)
arm_status | arm_rfft_init_q31 (arm_rfft_instance_q31 *S, arm_cfft_radix4_instance_q31 *S_CFFT, uint32_t fftLenReal, uint32_t ifftFlagR, uint32_t bitReverseFlag)
arm_status | arm_rfft_init_f32 (arm_rfft_instance_f32 *S, arm_cfft_radix4_instance_f32 *S_CFFT, uint32_t fftLenReal, uint32_t ifftFlagR, uint32_t bitReverseFlag)
void | arm_rfft_f32 (const arm_rfft_instance_f32 *S, float32_t *pSrc, float32_t *pDst)
arm_status | arm_dct4_init_f32 (arm_dct4_instance_f32 *S, arm_rfft_instance_f32 *S_RFFT, arm_cfft_radix4_instance_f32 *S_CFFT, uint16_t N, uint16_t Nby2, float32_t normalize)
void | arm_dct4_f32 (const arm_dct4_instance_f32 *S, float32_t *pState, float32_t *pInlineBuffer)
arm_status | arm_dct4_init_q31 (arm_dct4_instance_q31 *S, arm_rfft_instance_q31 *S_RFFT, arm_cfft_radix4_instance_q31 *S_CFFT, uint16_t N, uint16_t Nby2, q31_t normalize)
void | arm_dct4_q31 (const arm_dct4_instance_q31 *S, q31_t *pState, q31_t *pInlineBuffer)
arm_status | arm_dct4_init_q15 (arm_dct4_instance_q15 *S, arm_rfft_instance_q15 *S_RFFT, arm_cfft_radix4_instance_q15 *S_CFFT, uint16_t N, uint16_t Nby2, q15_t normalize)
void | arm_dct4_q15 (const arm_dct4_instance_q15 *S, q15_t *pState, q15_t *pInlineBuffer)
void | arm_add_f32 (float32_t *pSrcA, float32_t *pSrcB, float32_t *pDst, uint32_t blockSize)
void | arm_add_q7 (q7_t *pSrcA, q7_t *pSrcB, q7_t *pDst, uint32_t blockSize)
void | arm_add_q15 (q15_t *pSrcA, q15_t *pSrcB, q15_t *pDst, uint32_t blockSize)
void | arm_add_q31 (q31_t *pSrcA, q31_t *pSrcB, q31_t *pDst, uint32_t blockSize)
void | arm_sub_f32 (float32_t *pSrcA, float32_t *pSrcB, float32_t *pDst, uint32_t blockSize)
void | arm_sub_q7 (q7_t *pSrcA, q7_t *pSrcB, q7_t *pDst, uint32_t blockSize)
void | arm_sub_q15 (q15_t *pSrcA, q15_t *pSrcB, q15_t *pDst, uint32_t blockSize)
void | arm_sub_q31 (q31_t *pSrcA, q31_t *pSrcB, q31_t *pDst, uint32_t blockSize)
void | arm_scale_f32 (float32_t *pSrc, float32_t scale, float32_t *pDst, uint32_t blockSize)
void | arm_scale_q7 (q7_t *pSrc, q7_t scaleFract, int8_t shift, q7_t *pDst, uint32_t blockSize)
void | arm_scale_q15 (q15_t *pSrc, q15_t scaleFract, int8_t shift, q15_t *pDst, uint32_t blockSize)
void | arm_scale_q31 (q31_t *pSrc, q31_t scaleFract, int8_t shift, q31_t *pDst, uint32_t blockSize)
void | arm_abs_q7 (q7_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_abs_f32 (float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_abs_q15 (q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_abs_q31 (q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_dot_prod_f32 (float32_t *pSrcA, float32_t *pSrcB, uint32_t blockSize, float32_t *result)
void | arm_dot_prod_q7 (q7_t *pSrcA, q7_t *pSrcB, uint32_t blockSize, q31_t *result)
void | arm_dot_prod_q15 (q15_t *pSrcA, q15_t *pSrcB, uint32_t blockSize, q63_t *result)
void | arm_dot_prod_q31 (q31_t *pSrcA, q31_t *pSrcB, uint32_t blockSize, q63_t *result)
void | arm_shift_q7 (q7_t *pSrc, int8_t shiftBits, q7_t *pDst, uint32_t blockSize)
void | arm_shift_q15 (q15_t *pSrc, int8_t shiftBits, q15_t *pDst, uint32_t blockSize)
void | arm_shift_q31 (q31_t *pSrc, int8_t shiftBits, q31_t *pDst, uint32_t blockSize)
void | arm_offset_f32 (float32_t *pSrc, float32_t offset, float32_t *pDst, uint32_t blockSize)
void | arm_offset_q7 (q7_t *pSrc, q7_t offset, q7_t *pDst, uint32_t blockSize)
void | arm_offset_q15 (q15_t *pSrc, q15_t offset, q15_t *pDst, uint32_t blockSize)
void | arm_offset_q31 (q31_t *pSrc, q31_t offset, q31_t *pDst, uint32_t blockSize)
void | arm_negate_f32 (float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_negate_q7 (q7_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_negate_q15 (q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_negate_q31 (q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_copy_f32 (float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_copy_q7 (q7_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_copy_q15 (q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_copy_q31 (q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_fill_f32 (float32_t value, float32_t *pDst, uint32_t blockSize)
void | arm_fill_q7 (q7_t value, q7_t *pDst, uint32_t blockSize)
void | arm_fill_q15 (q15_t value, q15_t *pDst, uint32_t blockSize)
void | arm_fill_q31 (q31_t value, q31_t *pDst, uint32_t blockSize)
void | arm_conv_f32 (float32_t *pSrcA, uint32_t srcALen, float32_t *pSrcB, uint32_t srcBLen, float32_t *pDst)
void | arm_conv_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst)
void | arm_conv_fast_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst)
void | arm_conv_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst)
void | arm_conv_fast_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst)
void | arm_conv_q7 (q7_t *pSrcA, uint32_t srcALen, q7_t *pSrcB, uint32_t srcBLen, q7_t *pDst)
arm_status | arm_conv_partial_f32 (float32_t *pSrcA, uint32_t srcALen, float32_t *pSrcB, uint32_t srcBLen, float32_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_fast_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_fast_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst, uint32_t firstIndex, uint32_t numPoints)
arm_status | arm_conv_partial_q7 (q7_t *pSrcA, uint32_t srcALen, q7_t *pSrcB, uint32_t srcBLen, q7_t *pDst, uint32_t firstIndex, uint32_t numPoints)
void | arm_fir_decimate_f32 (const arm_fir_decimate_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
arm_status | arm_fir_decimate_init_f32 (arm_fir_decimate_instance_f32 *S, uint16_t numTaps, uint8_t M, float32_t *pCoeffs, float32_t *pState, uint32_t blockSize)
void | arm_fir_decimate_q15 (const arm_fir_decimate_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_fir_decimate_fast_q15 (const arm_fir_decimate_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
arm_status | arm_fir_decimate_init_q15 (arm_fir_decimate_instance_q15 *S, uint16_t numTaps, uint8_t M, q15_t *pCoeffs, q15_t *pState, uint32_t blockSize)
void | arm_fir_decimate_q31 (const arm_fir_decimate_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_fir_decimate_fast_q31 (arm_fir_decimate_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
arm_status | arm_fir_decimate_init_q31 (arm_fir_decimate_instance_q31 *S, uint16_t numTaps, uint8_t M, q31_t *pCoeffs, q31_t *pState, uint32_t blockSize)
void | arm_fir_interpolate_q15 (const arm_fir_interpolate_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
arm_status | arm_fir_interpolate_init_q15 (arm_fir_interpolate_instance_q15 *S, uint8_t L, uint16_t numTaps, q15_t *pCoeffs, q15_t *pState, uint32_t blockSize)
void | arm_fir_interpolate_q31 (const arm_fir_interpolate_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
arm_status | arm_fir_interpolate_init_q31 (arm_fir_interpolate_instance_q31 *S, uint8_t L, uint16_t numTaps, q31_t *pCoeffs, q31_t *pState, uint32_t blockSize)
void | arm_fir_interpolate_f32 (const arm_fir_interpolate_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
arm_status | arm_fir_interpolate_init_f32 (arm_fir_interpolate_instance_f32 *S, uint8_t L, uint16_t numTaps, float32_t *pCoeffs, float32_t *pState, uint32_t blockSize)
void | arm_biquad_cas_df1_32x64_q31 (const arm_biquad_cas_df1_32x64_ins_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_biquad_cas_df1_32x64_init_q31 (arm_biquad_cas_df1_32x64_ins_q31 *S, uint8_t numStages, q31_t *pCoeffs, q63_t *pState, uint8_t postShift)
void | arm_biquad_cascade_df2T_f32 (const arm_biquad_cascade_df2T_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_biquad_cascade_df2T_init_f32 (arm_biquad_cascade_df2T_instance_f32 *S, uint8_t numStages, float32_t *pCoeffs, float32_t *pState)
void | arm_fir_lattice_init_q15 (arm_fir_lattice_instance_q15 *S, uint16_t numStages, q15_t *pCoeffs, q15_t *pState)
void | arm_fir_lattice_q15 (const arm_fir_lattice_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_fir_lattice_init_q31 (arm_fir_lattice_instance_q31 *S, uint16_t numStages, q31_t *pCoeffs, q31_t *pState)
void | arm_fir_lattice_q31 (const arm_fir_lattice_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_fir_lattice_init_f32 (arm_fir_lattice_instance_f32 *S, uint16_t numStages, float32_t *pCoeffs, float32_t *pState)
void | arm_fir_lattice_f32 (const arm_fir_lattice_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_iir_lattice_f32 (const arm_iir_lattice_instance_f32 *S, float32_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_iir_lattice_init_f32 (arm_iir_lattice_instance_f32 *S, uint16_t numStages, float32_t *pkCoeffs, float32_t *pvCoeffs, float32_t *pState, uint32_t blockSize)
void | arm_iir_lattice_q31 (const arm_iir_lattice_instance_q31 *S, q31_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_iir_lattice_init_q31 (arm_iir_lattice_instance_q31 *S, uint16_t numStages, q31_t *pkCoeffs, q31_t *pvCoeffs, q31_t *pState, uint32_t blockSize)
void | arm_iir_lattice_q15 (const arm_iir_lattice_instance_q15 *S, q15_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_iir_lattice_init_q15 (arm_iir_lattice_instance_q15 *S, uint16_t numStages, q15_t *pkCoeffs, q15_t *pvCoeffs, q15_t *pState, uint32_t blockSize)
void | arm_lms_f32 (const arm_lms_instance_f32 *S, float32_t *pSrc, float32_t *pRef, float32_t *pOut, float32_t *pErr, uint32_t blockSize)
void | arm_lms_init_f32 (arm_lms_instance_f32 *S, uint16_t numTaps, float32_t *pCoeffs, float32_t *pState, float32_t mu, uint32_t blockSize)
void | arm_lms_init_q15 (arm_lms_instance_q15 *S, uint16_t numTaps, q15_t *pCoeffs, q15_t *pState, q15_t mu, uint32_t blockSize, uint32_t postShift)
void | arm_lms_q15 (const arm_lms_instance_q15 *S, q15_t *pSrc, q15_t *pRef, q15_t *pOut, q15_t *pErr, uint32_t blockSize)
void | arm_lms_q31 (const arm_lms_instance_q31 *S, q31_t *pSrc, q31_t *pRef, q31_t *pOut, q31_t *pErr, uint32_t blockSize)
void | arm_lms_init_q31 (arm_lms_instance_q31 *S, uint16_t numTaps, q31_t *pCoeffs, q31_t *pState, q31_t mu, uint32_t blockSize, uint32_t postShift)
void | arm_lms_norm_f32 (arm_lms_norm_instance_f32 *S, float32_t *pSrc, float32_t *pRef, float32_t *pOut, float32_t *pErr, uint32_t blockSize)
void | arm_lms_norm_init_f32 (arm_lms_norm_instance_f32 *S, uint16_t numTaps, float32_t *pCoeffs, float32_t *pState, float32_t mu, uint32_t blockSize)
void | arm_lms_norm_q31 (arm_lms_norm_instance_q31 *S, q31_t *pSrc, q31_t *pRef, q31_t *pOut, q31_t *pErr, uint32_t blockSize)
void | arm_lms_norm_init_q31 (arm_lms_norm_instance_q31 *S, uint16_t numTaps, q31_t *pCoeffs, q31_t *pState, q31_t mu, uint32_t blockSize, uint8_t postShift)
void | arm_lms_norm_q15 (arm_lms_norm_instance_q15 *S, q15_t *pSrc, q15_t *pRef, q15_t *pOut, q15_t *pErr, uint32_t blockSize)
void | arm_lms_norm_init_q15 (arm_lms_norm_instance_q15 *S, uint16_t numTaps, q15_t *pCoeffs, q15_t *pState, q15_t mu, uint32_t blockSize, uint8_t postShift)
void | arm_correlate_f32 (float32_t *pSrcA, uint32_t srcALen, float32_t *pSrcB, uint32_t srcBLen, float32_t *pDst)
void | arm_correlate_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst)
void | arm_correlate_fast_q15 (q15_t *pSrcA, uint32_t srcALen, q15_t *pSrcB, uint32_t srcBLen, q15_t *pDst)
void | arm_correlate_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst)
void | arm_correlate_fast_q31 (q31_t *pSrcA, uint32_t srcALen, q31_t *pSrcB, uint32_t srcBLen, q31_t *pDst)
void | arm_correlate_q7 (q7_t *pSrcA, uint32_t srcALen, q7_t *pSrcB, uint32_t srcBLen, q7_t *pDst)
void | arm_fir_sparse_f32 (arm_fir_sparse_instance_f32 *S, float32_t *pSrc, float32_t *pDst, float32_t *pScratchIn, uint32_t blockSize)
void | arm_fir_sparse_init_f32 (arm_fir_sparse_instance_f32 *S, uint16_t numTaps, float32_t *pCoeffs, float32_t *pState, int32_t *pTapDelay, uint16_t maxDelay, uint32_t blockSize)
void | arm_fir_sparse_q31 (arm_fir_sparse_instance_q31 *S, q31_t *pSrc, q31_t *pDst, q31_t *pScratchIn, uint32_t blockSize)
void | arm_fir_sparse_init_q31 (arm_fir_sparse_instance_q31 *S, uint16_t numTaps, q31_t *pCoeffs, q31_t *pState, int32_t *pTapDelay, uint16_t maxDelay, uint32_t blockSize)
void | arm_fir_sparse_q15 (arm_fir_sparse_instance_q15 *S, q15_t *pSrc, q15_t *pDst, q15_t *pScratchIn, q31_t *pScratchOut, uint32_t blockSize)
void | arm_fir_sparse_init_q15 (arm_fir_sparse_instance_q15 *S, uint16_t numTaps, q15_t *pCoeffs, q15_t *pState, int32_t *pTapDelay, uint16_t maxDelay, uint32_t blockSize)
void | arm_fir_sparse_q7 (arm_fir_sparse_instance_q7 *S, q7_t *pSrc, q7_t *pDst, q7_t *pScratchIn, q31_t *pScratchOut, uint32_t blockSize)
void | arm_fir_sparse_init_q7 (arm_fir_sparse_instance_q7 *S, uint16_t numTaps, q7_t *pCoeffs, q7_t *pState, int32_t *pTapDelay, uint16_t maxDelay, uint32_t blockSize)
void | arm_sin_cos_f32 (float32_t theta, float32_t *pSinVal, float32_t *pCcosVal)
void | arm_sin_cos_q31 (q31_t theta, q31_t *pSinVal, q31_t *pCosVal)
void | arm_cmplx_conj_f32 (float32_t *pSrc, float32_t *pDst, uint32_t numSamples)
void | arm_cmplx_conj_q31 (q31_t *pSrc, q31_t *pDst, uint32_t numSamples)
void | arm_cmplx_conj_q15 (q15_t *pSrc, q15_t *pDst, uint32_t numSamples)
void | arm_cmplx_mag_squared_f32 (float32_t *pSrc, float32_t *pDst, uint32_t numSamples)
void | arm_cmplx_mag_squared_q31 (q31_t *pSrc, q31_t *pDst, uint32_t numSamples)
void | arm_cmplx_mag_squared_q15 (q15_t *pSrc, q15_t *pDst, uint32_t numSamples)
static __INLINE float32_t | arm_pid_f32 (arm_pid_instance_f32 *S, float32_t in)
static __INLINE q31_t | arm_pid_q31 (arm_pid_instance_q31 *S, q31_t in)
static __INLINE q15_t | arm_pid_q15 (arm_pid_instance_q15 *S, q15_t in)
arm_status | arm_mat_inverse_f32 (const arm_matrix_instance_f32 *src, arm_matrix_instance_f32 *dst)
static __INLINE void | arm_clarke_f32 (float32_t Ia, float32_t Ib, float32_t *pIalpha, float32_t *pIbeta)
static __INLINE void | arm_clarke_q31 (q31_t Ia, q31_t Ib, q31_t *pIalpha, q31_t *pIbeta)
void | arm_q7_to_q31 (q7_t *pSrc, q31_t *pDst, uint32_t blockSize)
static __INLINE void | arm_inv_clarke_f32 (float32_t Ialpha, float32_t Ibeta, float32_t *pIa, float32_t *pIb)
static __INLINE void | arm_inv_clarke_q31 (q31_t Ialpha, q31_t Ibeta, q31_t *pIa, q31_t *pIb)
void | arm_q7_to_q15 (q7_t *pSrc, q15_t *pDst, uint32_t blockSize)
static __INLINE void | arm_park_f32 (float32_t Ialpha, float32_t Ibeta, float32_t *pId, float32_t *pIq, float32_t sinVal, float32_t cosVal)
static __INLINE void | arm_park_q31 (q31_t Ialpha, q31_t Ibeta, q31_t *pId, q31_t *pIq, q31_t sinVal, q31_t cosVal)
void | arm_q7_to_float (q7_t *pSrc, float32_t *pDst, uint32_t blockSize)
static __INLINE void | arm_inv_park_f32 (float32_t Id, float32_t Iq, float32_t *pIalpha, float32_t *pIbeta, float32_t sinVal, float32_t cosVal)
static __INLINE void | arm_inv_park_q31 (q31_t Id, q31_t Iq, q31_t *pIalpha, q31_t *pIbeta, q31_t sinVal, q31_t cosVal)
void | arm_q31_to_float (q31_t *pSrc, float32_t *pDst, uint32_t blockSize)
static __INLINE float32_t | arm_linear_interp_f32 (arm_linear_interp_instance_f32 *S, float32_t x)
static __INLINE q31_t | arm_linear_interp_q31 (q31_t *pYData, q31_t x, uint32_t nValues)
static __INLINE q15_t | arm_linear_interp_q15 (q15_t *pYData, q31_t x, uint32_t nValues)
static __INLINE q7_t | arm_linear_interp_q7 (q7_t *pYData, q31_t x, uint32_t nValues)
float32_t | arm_sin_f32 (float32_t x)
q31_t | arm_sin_q31 (q31_t x)
q15_t | arm_sin_q15 (q15_t x)
float32_t | arm_cos_f32 (float32_t x)
q31_t | arm_cos_q31 (q31_t x)
q15_t | arm_cos_q15 (q15_t x)
static __INLINE arm_status | arm_sqrt_f32 (float32_t in, float32_t *pOut)
arm_status | arm_sqrt_q31 (q31_t in, q31_t *pOut)
arm_status | arm_sqrt_q15 (q15_t in, q15_t *pOut)
static __INLINE void | arm_circularWrite_f32 (int32_t *circBuffer, int32_t L, uint16_t *writeOffset, int32_t bufferInc, const int32_t *src, int32_t srcInc, uint32_t blockSize)
static __INLINE void | arm_circularRead_f32 (int32_t *circBuffer, int32_t L, int32_t *readOffset, int32_t bufferInc, int32_t *dst, int32_t *dst_base, int32_t dst_length, int32_t dstInc, uint32_t blockSize)
static __INLINE void | arm_circularWrite_q15 (q15_t *circBuffer, int32_t L, uint16_t *writeOffset, int32_t bufferInc, const q15_t *src, int32_t srcInc, uint32_t blockSize)
static __INLINE void | arm_circularRead_q15 (q15_t *circBuffer, int32_t L, int32_t *readOffset, int32_t bufferInc, q15_t *dst, q15_t *dst_base, int32_t dst_length, int32_t dstInc, uint32_t blockSize)
static __INLINE void | arm_circularWrite_q7 (q7_t *circBuffer, int32_t L, uint16_t *writeOffset, int32_t bufferInc, const q7_t *src, int32_t srcInc, uint32_t blockSize)
static __INLINE void | arm_circularRead_q7 (q7_t *circBuffer, int32_t L, int32_t *readOffset, int32_t bufferInc, q7_t *dst, q7_t *dst_base, int32_t dst_length, int32_t dstInc, uint32_t blockSize)
void | arm_power_q31 (q31_t *pSrc, uint32_t blockSize, q63_t *pResult)
void | arm_power_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult)
void | arm_power_q15 (q15_t *pSrc, uint32_t blockSize, q63_t *pResult)
void | arm_power_q7 (q7_t *pSrc, uint32_t blockSize, q31_t *pResult)
void | arm_mean_q7 (q7_t *pSrc, uint32_t blockSize, q7_t *pResult)
void | arm_mean_q15 (q15_t *pSrc, uint32_t blockSize, q15_t *pResult)
void | arm_mean_q31 (q31_t *pSrc, uint32_t blockSize, q31_t *pResult)
void | arm_mean_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult)
void | arm_var_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult)
void | arm_var_q31 (q31_t *pSrc, uint32_t blockSize, q63_t *pResult)
void | arm_var_q15 (q15_t *pSrc, uint32_t blockSize, q31_t *pResult)
void | arm_rms_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult)
void | arm_rms_q31 (q31_t *pSrc, uint32_t blockSize, q31_t *pResult)
void | arm_rms_q15 (q15_t *pSrc, uint32_t blockSize, q15_t *pResult)
void | arm_std_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult)
void | arm_std_q31 (q31_t *pSrc, uint32_t blockSize, q31_t *pResult)
void | arm_std_q15 (q15_t *pSrc, uint32_t blockSize, q15_t *pResult)
void | arm_cmplx_mag_f32 (float32_t *pSrc, float32_t *pDst, uint32_t numSamples)
void | arm_cmplx_mag_q31 (q31_t *pSrc, q31_t *pDst, uint32_t numSamples)
void | arm_cmplx_mag_q15 (q15_t *pSrc, q15_t *pDst, uint32_t numSamples)
void | arm_cmplx_dot_prod_q15 (q15_t *pSrcA, q15_t *pSrcB, uint32_t numSamples, q31_t *realResult, q31_t *imagResult)
void | arm_cmplx_dot_prod_q31 (q31_t *pSrcA, q31_t *pSrcB, uint32_t numSamples, q63_t *realResult, q63_t *imagResult)
void | arm_cmplx_dot_prod_f32 (float32_t *pSrcA, float32_t *pSrcB, uint32_t numSamples, float32_t *realResult, float32_t *imagResult)
void | arm_cmplx_mult_real_q15 (q15_t *pSrcCmplx, q15_t *pSrcReal, q15_t *pCmplxDst, uint32_t numSamples)
void | arm_cmplx_mult_real_q31 (q31_t *pSrcCmplx, q31_t *pSrcReal, q31_t *pCmplxDst, uint32_t numSamples)
void | arm_cmplx_mult_real_f32 (float32_t *pSrcCmplx, float32_t *pSrcReal, float32_t *pCmplxDst, uint32_t numSamples)
void | arm_min_q7 (q7_t *pSrc, uint32_t blockSize, q7_t *result, uint32_t *index)
void | arm_min_q15 (q15_t *pSrc, uint32_t blockSize, q15_t *pResult, uint32_t *pIndex)
void | arm_min_q31 (q31_t *pSrc, uint32_t blockSize, q31_t *pResult, uint32_t *pIndex)
void | arm_min_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult, uint32_t *pIndex)
void | arm_max_q7 (q7_t *pSrc, uint32_t blockSize, q7_t *pResult, uint32_t *pIndex)
void | arm_max_q15 (q15_t *pSrc, uint32_t blockSize, q15_t *pResult, uint32_t *pIndex)
void | arm_max_q31 (q31_t *pSrc, uint32_t blockSize, q31_t *pResult, uint32_t *pIndex)
void | arm_max_f32 (float32_t *pSrc, uint32_t blockSize, float32_t *pResult, uint32_t *pIndex)
void | arm_cmplx_mult_cmplx_q15 (q15_t *pSrcA, q15_t *pSrcB, q15_t *pDst, uint32_t numSamples)
void | arm_cmplx_mult_cmplx_q31 (q31_t *pSrcA, q31_t *pSrcB, q31_t *pDst, uint32_t numSamples)
void | arm_cmplx_mult_cmplx_f32 (float32_t *pSrcA, float32_t *pSrcB, float32_t *pDst, uint32_t numSamples)
void | arm_float_to_q31 (float32_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_float_to_q15 (float32_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_float_to_q7 (float32_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_q31_to_q15 (q31_t *pSrc, q15_t *pDst, uint32_t blockSize)
void | arm_q31_to_q7 (q31_t *pSrc, q7_t *pDst, uint32_t blockSize)
void | arm_q15_to_float (q15_t *pSrc, float32_t *pDst, uint32_t blockSize)
void | arm_q15_to_q31 (q15_t *pSrc, q31_t *pDst, uint32_t blockSize)
void | arm_q15_to_q7 (q15_t *pSrc, q7_t *pDst, uint32_t blockSize)
static __INLINE float32_t | arm_bilinear_interp_f32 (const arm_bilinear_interp_instance_f32 *S, float32_t X, float32_t Y)
static __INLINE q31_t | arm_bilinear_interp_q31 (arm_bilinear_interp_instance_q31 *S, q31_t X, q31_t Y)
static __INLINE q15_t | arm_bilinear_interp_q15 (arm_bilinear_interp_instance_q15 *S, q31_t X, q31_t Y)
static __INLINE q7_t | arm_bilinear_interp_q7 (arm_bilinear_interp_instance_q7 *S, q31_t X, q31_t Y)

## Define Documentation

#define __CMSIS_GENERIC

Definition at line 254 of file arm_math.h.

#define DELTA_Q31 (0x100)

Macros required for reciprocal calculation in Normalized LMS.

Definition at line 280 of file arm_math.h.

#define DELTA_Q15 0x5

Definition at line 281 of file arm_math.h.

#define INDEX_MASK 0x0000003F

Definition at line 282 of file arm_math.h.

#define PI 3.14159265358979f

Definition at line 283 of file arm_math.h.

#define TABLE_SIZE 256

Macros required for SINE and COSINE Fast math approximations.

Definition at line 289 of file arm_math.h.

#define TABLE_SPACING_Q31 0x800000

Definition at line 290 of file arm_math.h.

#define TABLE_SPACING_Q15 0x80

Definition at line 291 of file arm_math.h.

#define INPUT_SPACING 0xB60B61

Macros required for SINE and COSINE Controller functions.

Definition at line 298 of file arm_math.h.

#define __SIMD32 | ( |  | addr ) | (*(int32_t **) & (addr))

definition to read/write two 16 bit values.

Definition at line 349 of file arm_math.h.

#define __PACKq7 | ( |  | v0,
|  |  | v1,
|  |  | v2,
|  |  | v3
| ) |  |

Value:

    ( (((int32_t)(v0) <<  0) & (int32_t)0x000000FF) |   \
                                    (((int32_t)(v1) <<  8) & (int32_t)0x0000FF00) | \
                                    (((int32_t)(v2) << 16) & (int32_t)0x00FF0000) | \
                                    (((int32_t)(v3) << 24) & (int32_t)0xFF000000)  )

definition to pack four 8 bit values.

Definition at line 366 of file arm_math.h.

## Typedef Documentation

typedef int8_t q7_t

8-bit fractional data type in 1.7 format.

Definition at line 319 of file arm_math.h.

typedef int16_t q15_t

16-bit fractional data type in 1.15 format.

Definition at line 324 of file arm_math.h.

typedef int32_t q31_t

32-bit fractional data type in 1.31 format.

Definition at line 329 of file arm_math.h.

typedef int64_t q63_t

64-bit fractional data type in 1.63 format.

Definition at line 334 of file arm_math.h.

typedef float float32_t

32-bit floating-point type definition.

Definition at line 339 of file arm_math.h.

typedef double float64_t

64-bit floating-point type definition.

Definition at line 344 of file arm_math.h.

## Enumeration Type Documentation

enum arm_status

Error status returned by some functions in the library.

Enumerator:

  ARM_MATH_SUCCESS | No error
  ARM_MATH_ARGUMENT_ERROR | One or more arguments are incorrect
  ARM_MATH_LENGTH_ERROR | Length of data buffer is incorrect
  ARM_MATH_SIZE_MISMATCH | Size of matrices is not compatible with the operation.
  ARM_MATH_NANINF | Not-a-number (NaN) or infinity is generated
  ARM_MATH_SINGULAR | Generated by matrix inversion if the input matrix is singular and cannot be inverted.
  ARM_MATH_TEST_FAILURE | Test Failed

Definition at line 305 of file arm_math.h.

## Function Documentation

static __INLINE q31_t clip_q63_to_q31 | ( | q63_t | x ) | `[static]`

Clips Q63 to Q31 values.

Definition at line 383 of file arm_math.h.

static __INLINE q15_t clip_q63_to_q15 | ( | q63_t | x ) | `[static]`

Clips Q63 to Q15 values.

Definition at line 393 of file arm_math.h.

static __INLINE q7_t clip_q31_to_q7 | ( | q31_t | x ) | `[static]`

Clips Q31 to Q7 values.

Definition at line 403 of file arm_math.h.

static __INLINE q15_t clip_q31_to_q15 | ( | q31_t | x ) | `[static]`

Clips Q31 to Q15 values.

Definition at line 413 of file arm_math.h.

static __INLINE q63_t mult32x64 | ( | q63_t | x,
|  | q31_t | y
| ) |  | `[static]`

Multiplies 32 X 64 and returns 32 bit result in 2.30 format.

Definition at line 424 of file arm_math.h.

static __INLINE uint32_t arm_recip_q31 | ( | q31_t | in,
|  | q31_t * | dst,
|  | q31_t * | pRecipTable
| ) |  | `[static]`

Function to Calculates 1/in(reciprocal) value of Q31 Data type.

Definition at line 463 of file arm_math.h.

static __INLINE uint32_t arm_recip_q15 | ( | q15_t | in,
|  | q15_t * | dst,
|  | q15_t * | pRecipTable
| ) |  | `[static]`

Function to Calculates 1/in(reciprocal) value of Q15 Data type.

Definition at line 514 of file arm_math.h.

void arm_radix4_butterfly_f32 | ( | float32_t * | pSrc,
|  | uint16_t | fftLen,
|  | float32_t * | pCoef,
|  | uint16_t | twidCoefModifier
| ) |  |

Core function for the floating-point CFFT butterfly process.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of floating-point data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef | points to the twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

end of CFFT_CIFFT group

Definition at line 223 of file arm_cfft_radix4_f32.c.

void arm_radix4_butterfly_inverse_f32 | ( | float32_t * | pSrc,
|  | uint16_t | fftLen,
|  | float32_t * | pCoef,
|  | uint16_t | twidCoefModifier,
|  | float32_t | onebyfftLen
| ) |  |

Core function for the floating-point CIFFT butterfly process.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of floating-point data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.
  [in] | onebyfftLen | value of 1/fftLen.

Returns:
  none.

Definition at line 660 of file arm_cfft_radix4_f32.c.

void arm_bitreversal_f32 | ( | float32_t * | pSrc,
|  | uint16_t | fftSize,
|  | uint16_t | bitRevFactor,
|  | uint16_t * | pBitRevTab
| ) |  |

In-place bit reversal function.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of floating-point data type.
  [in] | fftSize | length of the FFT.
  [in] | bitRevFactor | bit reversal modifier that supports different size FFTs with the same bit reversal table.
  [in] | *pBitRevTab | points to the bit reversal table.

Returns:
  none.

Definition at line 1177 of file arm_cfft_radix4_f32.c.

void arm_radix4_butterfly_q31 | ( | q31_t * | pSrc,
|  | uint32_t | fftLen,
|  | q31_t * | pCoef,
|  | uint32_t | twidCoefModifier
| ) |  |

Core function for the Q31 CFFT butterfly process.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of Q31 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

end of CFFT_CIFFT group

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of Q31 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

Definition at line 139 of file arm_cfft_radix4_q31.c.

void arm_radix4_butterfly_inverse_q31 | ( | q31_t * | pSrc,
|  | uint32_t | fftLen,
|  | q31_t * | pCoef,
|  | uint32_t | twidCoefModifier
| ) |  |

Core function for the Q31 CIFFT butterfly process.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of Q31 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

Definition at line 517 of file arm_cfft_radix4_q31.c.

void arm_bitreversal_q31 | ( | q31_t * | pSrc,
|  | uint32_t | fftLen,
|  | uint16_t | bitRevFactor,
|  | uint16_t * | pBitRevTab
| ) |  |

In-place bit reversal function.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of Q31 data type.
  [in] | fftLen | length of the FFT.
  [in] | bitRevFactor | bit reversal modifier that supports different size FFTs with the same bit reversal table
  [in] | *pBitRevTab | points to bit reversal table.

Returns:
  none.

Definition at line 848 of file arm_cfft_radix4_q31.c.

void arm_radix4_butterfly_q15 | ( | q15_t * | pSrc16,
|  | uint32_t | fftLen,
|  | q15_t * | pCoef16,
|  | uint32_t | twidCoefModifier
| ) |  |

Core function for the Q15 CFFT butterfly process.

Parameters:

  [in,out] | *pSrc16 | points to the in-place buffer of Q15 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef16 | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

end of CFFT_CIFFT group

Parameters:

  [in,out] | *pSrc16 | points to the in-place buffer of Q15 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef16 | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

Definition at line 138 of file arm_cfft_radix4_q15.c.

void arm_radix4_butterfly_inverse_q15 | ( | q15_t * | pSrc16,
|  | uint32_t | fftLen,
|  | q15_t * | pCoef16,
|  | uint32_t | twidCoefModifier
| ) |  |

Core function for the Q15 CIFFT butterfly process.

Parameters:

  [in,out] | *pSrc16 | points to the in-place buffer of Q15 data type.
  [in] | fftLen | length of the FFT.
  [in] | *pCoef16 | points to twiddle coefficient buffer.
  [in] | twidCoefModifier | twiddle coefficient modifier that supports different size FFTs with the same twiddle factor table.

Returns:
  none.

Definition at line 1053 of file arm_cfft_radix4_q15.c.

void arm_bitreversal_q15 | ( | q15_t * | pSrc,
|  | uint32_t | fftLen,
|  | uint16_t | bitRevFactor,
|  | uint16_t * | pBitRevTab
| ) |  |

In-place bit reversal function.

Parameters:

  [in,out] | *pSrc | points to the in-place buffer of Q15 data type.
  [in] | fftLen | length of the FFT.
  [in] | bitRevFactor | bit reversal modifier that supports different size FFTs with the same bit reversal table
  [in] | *pBitRevTab | points to bit reversal table.

Returns:
  none.

Definition at line 1906 of file arm_cfft_radix4_q15.c.

static __INLINE void arm_circularWrite_f32 | ( | int32_t * | circBuffer,
|  | int32_t | L,
|  | uint16_t * | writeOffset,
|  | int32_t | bufferInc,
|  | const int32_t * | src,
|  | int32_t | srcInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

floating-point Circular write function.

end of SQRT group

Definition at line 5751 of file arm_math.h.

static __INLINE void arm_circularRead_f32 | ( | int32_t * | circBuffer,
|  | int32_t | L,
|  | int32_t * | readOffset,
|  | int32_t | bufferInc,
|  | int32_t * | dst,
|  | int32_t * | dst_base,
|  | int32_t | dst_length,
|  | int32_t | dstInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

floating-point Circular Read function.

Definition at line 5796 of file arm_math.h.

static __INLINE void arm_circularWrite_q15 | ( | q15_t * | circBuffer,
|  | int32_t | L,
|  | uint16_t * | writeOffset,
|  | int32_t | bufferInc,
|  | const q15_t * | src,
|  | int32_t | srcInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

Q15 Circular write function.

Definition at line 5851 of file arm_math.h.

static __INLINE void arm_circularRead_q15 | ( | q15_t * | circBuffer,
|  | int32_t | L,
|  | int32_t * | readOffset,
|  | int32_t | bufferInc,
|  | q15_t * | dst,
|  | q15_t * | dst_base,
|  | int32_t | dst_length,
|  | int32_t | dstInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

Q15 Circular Read function.

Definition at line 5896 of file arm_math.h.

static __INLINE void arm_circularWrite_q7 | ( | q7_t * | circBuffer,
|  | int32_t | L,
|  | uint16_t * | writeOffset,
|  | int32_t | bufferInc,
|  | const q7_t * | src,
|  | int32_t | srcInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

Q7 Circular write function.

Definition at line 5953 of file arm_math.h.

static __INLINE void arm_circularRead_q7 | ( | q7_t * | circBuffer,
|  | int32_t | L,
|  | int32_t * | readOffset,
|  | int32_t | bufferInc,
|  | q7_t * | dst,
|  | q7_t * | dst_base,
|  | int32_t | dst_length,
|  | int32_t | dstInc,
|  | uint32_t | blockSize
| ) |  | `[static]`

Q7 Circular Read function.

Definition at line 5998 of file arm_math.h.

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines