| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_RITIMER_001_T Struct Reference
IP: RITimer register block and driver

## Detailed Description

Repetitive Interrupt Timer register block structure.

Definition at line 51 of file ritimer_001.h.

`#include "ritimer_001.h"`

## Data Fields
__IO uint32_t | COMPVAL
__IO uint32_t | MASK
__IO uint32_t | CTRL
__IO uint32_t | COUNTER

## Field Documentation

__IO uint32_t COMPVAL

< RITIMER Structure Compare register

Definition at line 52 of file ritimer_001.h.

__IO uint32_t COUNTER

32-bit counter

Definition at line 55 of file ritimer_001.h.

__IO uint32_t CTRL

Control register.

Definition at line 54 of file ritimer_001.h.

__IO uint32_t MASK

Mask register. This register holds the 32-bit mask value. A 1 written to any bit will force a compare on the corresponding bit of the counter and compare register.

Definition at line 53 of file ritimer_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/ritimer_001.h