| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_001_T Struct Reference
IP: CAN register block and driver

## Detailed Description

CAN register block structure.

Definition at line 123 of file can_001.h.

`#include "can_001.h"`

## Data Fields
__IO uint32_t | MOD
__O uint32_t | CMR
__IO uint32_t | GSR
__I uint32_t | ICR
__IO uint32_t | IER
__IO uint32_t | BTR
__IO uint32_t | EWL
__I uint32_t | SR
__IO IP_CAN_001_RX_T | RX
__IO IP_CAN_001_TX_T | TX [3]

## Field Documentation

__IO uint32_t BTR

CAN Bus Timing Register

Definition at line 130 of file can_001.h.

__O uint32_t CMR

CAN Command Register

Definition at line 126 of file can_001.h.

__IO uint32_t EWL

CAN Error Warning Limit Register

Definition at line 131 of file can_001.h.

__IO uint32_t GSR

CAN Global Status Register

Definition at line 127 of file can_001.h.

__I uint32_t ICR

CAN Interrupt and Capture Register

Definition at line 128 of file can_001.h.

__IO uint32_t IER

CAN Interrupt Enable Register

Definition at line 129 of file can_001.h.

__IO uint32_t MOD

CAN Mode Register

Definition at line 125 of file can_001.h.

__IO IP_CAN_001_RX_T RX

CAN Receive Registers

Definition at line 133 of file can_001.h.

__I uint32_t SR

CAN Status Register

Definition at line 132 of file can_001.h.

__IO IP_CAN_001_TX_T TX[3]

CAN Transmit Registers

Definition at line 134 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h