| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
uart_8xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC8xx UART driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __UART_8XX_H_
33 #define __UART_8XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
55 STATIC INLINE void Chip_UART_ConfigData(LPC_USART_T *pUART, IP_UART_002_DATALEN_T Databits,
56 IP_UART_002_PARITY_T Parity,
57 IP_UART_002_STOPLEN_T Stopbits)
58 {
59 IP_UART_Config(pUART, Databits, Parity, Stopbits);
60 }
61
69 STATIC INLINE void Chip_UART_IntEnable(LPC_USART_T *pUART,
70 uint32_t UARTIntCfg,
71 FunctionalState NewState)
72 {
73 IP_UART_IntEnable(pUART, UARTIntCfg, NewState);
74 }
75
81 STATIC INLINE uint32_t Chip_UART_GetIntStatus(LPC_USART_T *pUART)
82 {
83 return IP_UART_GetIntStatus(pUART);
84 }
85
91 void Chip_UART_Init(LPC_USART_T *pUART);
92
99 void Chip_UART_SetBaudRate(LPC_USART_T *pUART, uint32_t baudrate);
100
107 Status Chip_UART_SendByte(LPC_USART_T *pUART, uint8_t data);
108
115 Status Chip_UART_ReceiveByte(LPC_USART_T *pUART, uint8_t *Data);
116
121 #ifdef __cplusplus
122 }
123 #endif
124
125 #endif /* __UART_8XX_H_ */