| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
LPC17xx/40xx IPERF Server example
Misc examples

## Detailed Description

Example description

This example demonstrates the iperf server functionality using LWIP stack.
To use the example, connect an ethernet cable to the board. The board will acquire an IP address via DHCP and you can ping the board at it's IP address.
From the host PC execute the iperf tool with following options:

- iperf -i 5 -c < Target IP address > -m
  It will display the Interval, Transfer size, bandwidth, etc

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC17xx/40xx example quickstart for Keil uVision4
LPC17xx/40xx example quickstart for IAR EWARM
LPC17xx/40xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Embedded Artists' LPC1788 Developer's Kit
Embedded Artists' LPC4088 Developer's Kit

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
static void | prvSetupHardware (void)
int | main (void)
| main routine for example_lwip_tcpecho_sa_17xx40xx

## Variables
static struct netif | lpc_netif

## Function Documentation

int main | ( | void |  | ) |

main routine for example_lwip_tcpecho_sa_17xx40xx

Main program body.

Returns
  Function should not exit.

Definition at line 117 of file main.c.

static void prvSetupHardware | ( | void |  | ) |
| static

Definition at line 97 of file main.c.

## Variable Documentation

struct netif lpc_netif
| static

Definition at line 86 of file main.c.