| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions
LPC18xx/43xx Memory tests
Peripheral examples

## Detailed Description

Example description
This example runs a few memory tests on external DRAM memory. The tests include walking 0 and 1, address and inverse address, and pattern tests.

These tests are meant to be run via a debugger inside IRAM and will not run standalone.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Macros
#define | DRAM_BASE_ADDRESS (uint32_t *) 0x28000000

## Functions
int | main (void)
| Main routine for example_memtest.

## Macro Definition Documentation

#define DRAM_BASE_ADDRESS (uint32_t *) 0x28000000

Definition at line 71 of file memtest.c.

## Function Documentation

int main | ( | void |  | ) |

Main routine for example_memtest.

Main program body.

Returns
  Nothing

Definition at line 96 of file memtest.c.