| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_ENET_002_MODULE_CTRL_T Struct Reference
IP: Ethernet register block and driver (002)

## Detailed Description

Ethernet Module Control register block structure.

Definition at line 114 of file enet_002.h.

`#include "enet_002.h"`

## Data Fields
__I uint32_t | INTSTATUS
__IO uint32_t | INTENABLE
__O uint32_t | INTCLEAR
__O uint32_t | INTSET
uint32_t | RESERVED
__IO uint32_t | POWERDOWN

## Field Documentation

__O uint32_t INTCLEAR

Interrupt clear register

Definition at line 117 of file enet_002.h.

__IO uint32_t INTENABLE

Interrupt enable register

Definition at line 116 of file enet_002.h.

__O uint32_t INTSET

Interrupt set register

Definition at line 118 of file enet_002.h.

__I uint32_t INTSTATUS

Interrupt status register

Definition at line 115 of file enet_002.h.

__IO uint32_t POWERDOWN

Power-down register

Definition at line 120 of file enet_002.h.

uint32_t RESERVED

Definition at line 119 of file enet_002.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/enet_002.h