| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
pmc_18xx_43xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC18xx/43xx Power Management Controller driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __PMC_18XX_43XX_H_
33 #define __PMC_18XX_43XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
44 /*
45 * @brief PMC power states
46 */
47 typedef enum CHIP_PMC_PWR_STATE {
48 PMC_DeepSleep = PMC_PWR_DEEP_SLEEP_MODE,
49 PMC_PowerDown = PMC_PWR_POWER_DOWN_MODE,
50 PMC_DeepPowerDown = PMC_PWR_DEEP_POWER_DOWN_MODE,
51 } CHIP_PMC_PWR_STATE_T;
52
57 void Chip_PMC_Sleep(void);
58
64 void Chip_PMC_Set_PwrState(CHIP_PMC_PWR_STATE_T PwrState);
65
70 #ifdef __cplusplus
71 }
72 #endif
73
74 #endif /* __PMC_18XX_43XX_H_ */