| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Device.h
Go to the documentation of this file.
1 /*
2 * @brief Common USB Device definitions for all architectures
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * Copyright(C) Dean Camera, 2011, 2012
7 * All rights reserved.
8 *
9 * @par
10 * Software that is described herein is for illustrative purposes only
11 * which provides customers with programming information regarding the
12 * LPC products. This software is supplied "AS IS" without any warranties of
13 * any kind, and NXP Semiconductors and its licensor disclaim any and
14 * all warranties, express or implied, including all implied warranties of
15 * merchantability, fitness for a particular purpose and non-infringement of
16 * intellectual property rights. NXP Semiconductors assumes no responsibility
17 * or liability for the use of the software, conveys no license or rights under any
18 * patent, copyright, mask work right, or any other intellectual property rights in
19 * or to any products. NXP Semiconductors reserves the right to make changes
20 * in the software without notification. NXP Semiconductors also makes no
21 * representation or warranty that such application will be suitable for the
22 * specified use without further testing or modification.
23 *
24 * @par
25 * Permission to use, copy, modify, and distribute this software and its
26 * documentation is hereby granted, under NXP Semiconductors' and its
27 * licensor's relevant copyrights in the software, without fee, provided that it
28 * is used in conjunction with NXP Semiconductors microcontrollers. This
29 * copyright, permission, and disclaimer notice must appear in all copies of
30 * this code.
31 */
32
43 #ifndef __USBDEVICE_H__
44 #define __USBDEVICE_H__
45
46 /* Includes: */
47 #include "../../../Common/Common.h"
48 #include "USBMode.h"
49 #include "StdDescriptors.h"
50 #include "USBInterrupt.h"
51 #include "Endpoint.h"
52
53 /* Enable C linkage for C++ Compilers: */
54 #if defined(__cplusplus)
55 extern "C" {
56 #endif
57
58 /* Preprocessor Checks: */
59 #if !defined(__INCLUDE_FROM_USB_DRIVER)
60 #error Do not include this file directly. Include lpcroot/libraries/LPCUSBlib/Drivers/USB/USB.h instead.
61 #endif
62
63 /* Public Interface - May be used in end-application: */
64 /* Enums: */
72 enum USB_Device_States_t
73 {
74 DEVICE_STATE_Unattached = 0,
77 DEVICE_STATE_Powered = 1,
81 DEVICE_STATE_Default = 2,
85 DEVICE_STATE_Addressed = 3,
89 DEVICE_STATE_Configured = 4,
93 DEVICE_STATE_Suspended = 5,
98 };
99
100 /* Function Prototypes: */
127 uint16_t CALLBACK_USB_GetDescriptor(uint8_t corenum, const uint16_t wValue,
128 const uint8_t wIndex,
129 const void** const DescriptorAddress
130 #if (defined(ARCH_HAS_MULTI_ADDRESS_SPACE) || defined(__DOXYGEN__)) && \
131 !(defined(USE_FLASH_DESCRIPTORS) || defined(USE_EEPROM_DESCRIPTORS) || defined(USE_RAM_DESCRIPTORS))
132 , uint8_t* MemoryAddressSpace
133 #endif
134 ) ATTR_WARN_UNUSED_RESULT ATTR_NON_NULL_PTR_ARG(4);
135
136 #if defined(__LPC18XX__) || defined(__LPC43XX__)
137 #include "DCD/LPC18XX/Device_LPC18xx.h"
138 #elif defined(__LPC175X_6X__) || defined(__LPC177X_8X__) || defined(__LPC407X_8X__)
139 #include "DCD/LPC17XX/Device_LPC17xx.h"
140 #elif defined(__LPC11U1X__) || defined(__LPC11U2X_3X__) || defined(__LPC1347__)
141 #include "DCD/LPC11UXX/Device_LPC11Uxx.h"
142 #endif
143
144 /* Disable C linkage for C++ Compilers: */
145 #if defined(__cplusplus)
146 }
147 #endif
148
149 #endif
150