| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_GIMA_001_T Struct Reference
IP: GIMA register block and driver

## Detailed Description

Global Input Multiplexer Array (GIMA) register block structure.

Definition at line 51 of file gima_001.h.

`#include "gima_001.h"`

## Data Fields
__IO uint32_t | CAP0_IN [4][4]
__IO uint32_t | CTIN_IN [8]
__IO uint32_t | VADC_TRIGGER_IN
__IO uint32_t | EVENTROUTER_13_IN
__IO uint32_t | EVENTROUTER_14_IN
__IO uint32_t | EVENTROUTER_16_IN
__IO uint32_t | ADCSTART0_IN
__IO uint32_t | ADCSTART1_IN

## Field Documentation

__IO uint32_t ADCSTART0_IN

ADC start0 input multiplexer (GIMA output 28)

Definition at line 58 of file gima_001.h.

__IO uint32_t ADCSTART1_IN

ADC start1 input multiplexer (GIMA output 29)

Definition at line 59 of file gima_001.h.

__IO uint32_t CAP0_IN[4][4]

< GIMA Structure Timer x CAP0_y capture input multiplexer (GIMA output ((x*4)+y))

Definition at line 52 of file gima_001.h.

__IO uint32_t CTIN_IN[8]

SCT CTIN_x capture input multiplexer (GIMA output (16+x))

Definition at line 53 of file gima_001.h.

__IO uint32_t EVENTROUTER_13_IN

Event router input 13 multiplexer (GIMA output 25)

Definition at line 55 of file gima_001.h.

__IO uint32_t EVENTROUTER_14_IN

Event router input 14 multiplexer (GIMA output 26)

Definition at line 56 of file gima_001.h.

__IO uint32_t EVENTROUTER_16_IN

Event router input 16 multiplexer (GIMA output 27)

Definition at line 57 of file gima_001.h.

__IO uint32_t VADC_TRIGGER_IN

VADC trigger input multiplexer (GIMA output 24)

Definition at line 54 of file gima_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/gima_001.h