| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
pmc_001.h
Go to the documentation of this file.
1 /*
2 * @brief Power Management Controller registers and control functions
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __PMC_001_H_
33 #define __PMC_001_H_
34
35 #include "sys_config.h"
36 #include "cmsis.h"
37
38 #ifdef __cplusplus
39 extern "C" {
40 #endif
41
50 typedef struct {
51 __IO uint32_t PD0_SLEEP0_HW_ENA;
52 __I uint32_t RESERVED0[6];
53 __IO uint32_t PD0_SLEEP0_MODE;
54 } IP_PMC_001_T;
55
59 #define PMC_PWR_DEEP_SLEEP_MODE 0x3F00AA
60 #define PMC_PWR_POWER_DOWN_MODE 0x3FFCBA
61 #define PMC_PWR_DEEP_POWER_DOWN_MODE 0x3FFF7F
62
69 STATIC INLINE void IP_PMC_SetPowerMode(IP_PMC_001_T *pPMC, uint32_t PwrMode)
70 {
71 pPMC->PD0_SLEEP0_MODE = PwrMode;
72 }
73
78 #ifdef __cplusplus
79 }
80 #endif
81
82 #endif /* __PMC_001_H_ */