| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
board_nxp_xpresso_1769.h
Go to the documentation of this file.
1 /*
2 * @brief NXP LPC1769 Xpresso board file
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __BOARD_NXP_XPRESSO_1769_H_
33 #define __BOARD_NXP_XPRESSO_1769_H_
34
35 #include "chip.h"
36 #include "board_api.h"
37 #include "lpc_phy.h"
38
39 #ifdef __cplusplus
40 extern "C" {
41 #endif
42
60 #define BOARD_NXP_XPRESSO_1769
65 #define LEDS_LED1 0x01
66 #define LEDS_LED2 0x02
67 #define LEDS_LED3 0x04
68 #define LEDS_LED4 0x08
69 #define LEDS_NO_LEDS 0x00
70
74 #define BUTTONS_BUTTON1 0x01
75 #define NO_BUTTON_PRESSED 0x00
76
80 #define JOY_UP 0x01
81 #define JOY_DOWN 0x02
82 #define JOY_LEFT 0x04
83 #define JOY_RIGHT 0x08
84 #define JOY_PRESS 0x10
85
89 #define MCB_17XX_AUDIO_MIC_SELECT 0x00
90 #define MCB_17XX_AUDIO_LINE_IN_SELECT 0x00
91
97 void Board_UART_Init(LPC_USART_T *pUART);
98
105 void Board_ENET_GetMacADDR(uint8_t *mcaddr);
106
112 void Board_Audio_Init(uint8_t audio_in_sel);
113
119 void Board_SSP_Init(LPC_SSP_T *pSSP);
120
126 void Board_SPI_Init(bool isMaster);
127
132 void Board_SPI_AssertSSEL(void);
133
138 void Board_SPI_DeassertSSEL(void);
139
145 void Board_I2C_Init(I2C_ID_T id);
146
156 STATIC INLINE void Board_I2C_EnableFastPlus(I2C_ID_T id)
157 {
158 Chip_IOCON_SetI2CPad(LPC_IOCON, I2CPADCFG_FAST_MODE_PLUS);
159 }
160
166 STATIC INLINE void Board_I2C_DisableFastPlus(I2C_ID_T id)
167 {
168 Chip_IOCON_SetI2CPad(LPC_IOCON, I2CPADCFG_STD_MODE);
169 }
170
175 void Board_Buttons_Init(void);
176
181 uint32_t Buttons_GetStatus(void);
182
187 void Board_Joystick_Init(void);
188
193 uint8_t Joystick_GetStatus(void);
194
200 void Serial_CreateStream(void *Stream);
201
206 #ifdef __cplusplus
207 }
208 #endif
209
210 #endif /* __BOARD_NXP_XPRESSO_1769_H_ */