| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_GPIO_002_T Struct Reference
IP: GPIO register block and driver (002)

## Detailed Description

GPIO port (GPIO_PORT) for LPC175x_6x, LPC177x_8x and LPC407x_8x.

Definition at line 54 of file gpio_002.h.

`#include "gpio_002.h"`

## Data Fields
__IO uint32_t | DIR
uint32_t | RESERVED0 [3]
__IO uint32_t | MASK
__IO uint32_t | PIN
__IO uint32_t | SET
__O uint32_t | CLR

## Field Documentation

__O uint32_t CLR

Offset 0x001C: Output Clear register using FIOMASK

Definition at line 60 of file gpio_002.h.

__IO uint32_t DIR

Offset 0x0000: GPIO Port Direction control register

Definition at line 55 of file gpio_002.h.

__IO uint32_t MASK

Offset 0x0010: GPIO Mask register

Definition at line 57 of file gpio_002.h.

__IO uint32_t PIN

Offset 0x0014: Pin value register using FIOMASK

Definition at line 58 of file gpio_002.h.

uint32_t RESERVED0[3]

Definition at line 56 of file gpio_002.h.

__IO uint32_t SET

Offset 0x0018: Output Set register using FIOMASK

Definition at line 59 of file gpio_002.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/gpio_002.h