| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_ENET_001_ENHTXDESC_T Struct Reference
IP: Ethernet register block and driver

## Detailed Description

Structure of a enhanced transmit descriptor (with timestamp)

Definition at line 419 of file enet_001.h.

`#include "enet_001.h"`

## Data Fields
__IO uint32_t | CTRLSTAT
__IO uint32_t | BSIZE
__IO uint32_t | B1ADD
__IO uint32_t | B2ADD
__IO uint32_t | TDES4
__IO uint32_t | TDES5
__IO uint32_t | TTSL
__IO uint32_t | TTSH

## Field Documentation

__IO uint32_t B1ADD

Buffer 1 address

Definition at line 422 of file enet_001.h.

__IO uint32_t B2ADD

Buffer 2 or next descriptor address

Definition at line 423 of file enet_001.h.

__IO uint32_t BSIZE

Buffer 1/2 byte counts

Definition at line 421 of file enet_001.h.

__IO uint32_t CTRLSTAT

TDES control and status word

Definition at line 420 of file enet_001.h.

__IO uint32_t TDES4

Reserved

Definition at line 424 of file enet_001.h.

__IO uint32_t TDES5

Reserved

Definition at line 425 of file enet_001.h.

__IO uint32_t TTSH

Timestamp value high

Definition at line 427 of file enet_001.h.

__IO uint32_t TTSL

Timestamp value low

Definition at line 426 of file enet_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/enet_001.h