| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_001_AF_T Struct Reference
IP: CAN register block and driver

## Detailed Description

CAN acceptance filter register block structure.

Definition at line 74 of file can_001.h.

`#include "can_001.h"`

## Data Fields
__IO uint32_t | AFMR
__IO uint32_t | ENDADDR [CANAF_RAM_SECTION_NUM]
__I uint32_t | LUTERRAD
__I uint32_t | LUTERR
__IO uint32_t | FCANIE
__IO uint32_t | FCANIC [2]

## Field Documentation

__IO uint32_t AFMR

Acceptance Filter Register

Definition at line 76 of file can_001.h.

__IO uint32_t ENDADDR[CANAF_RAM_SECTION_NUM]

Start/End Address Registers

Definition at line 77 of file can_001.h.

__IO uint32_t FCANIC[2]

FullCAN Interrupt and Capture Registers

Definition at line 81 of file can_001.h.

__IO uint32_t FCANIE

Global FullCANInterrupt Enable Register

Definition at line 80 of file can_001.h.

__I uint32_t LUTERR

LUT Error Register

Definition at line 79 of file can_001.h.

__I uint32_t LUTERRAD

LUT Error Address Register

Definition at line 78 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h