| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
dac_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx D/A conversion driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __DAC_17XX_40XX_H_
33 #define __DAC_17XX_40XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
51 void Chip_DAC_Init(LPC_DAC_T *pDAC);
52
58 STATIC INLINE void Chip_DAC_DeInit(LPC_DAC_T *pDAC) {}
59
66 STATIC INLINE void Chip_DAC_UpdateValue(LPC_DAC_T *pDAC, uint32_t dac_value)
67 {
68 IP_DAC_UpdateValue(pDAC, dac_value);
69 }
70
79 STATIC INLINE void Chip_DAC_SetBias(LPC_DAC_T *pDAC, uint32_t bias)
80 {
81 IP_DAC_SetBias(pDAC, bias);
82 }
83
94 STATIC INLINE void Chip_DAC_ConfigDAConverterControl(LPC_DAC_T *pDAC, uint32_t dacFlags)
95 {
96 IP_DAC_ConfigDAConverterControl(pDAC, dacFlags);
97 }
98
105 STATIC INLINE void Chip_DAC_SetDMATimeOut(LPC_DAC_T *pDAC, uint32_t time_out)
106 {
107 IP_DAC_SetDMATimeOut(pDAC, time_out);
108 }
109
115 STATIC INLINE IntStatus Chip_DAC_GetIntStatus(LPC_DAC_T *pDAC)
116 {
117 return IP_DAC_GetIntStatus(pDAC);
118 }
119
124 #ifdef __cplusplus
125 }
126 #endif
127
128 #endif /* __DAC_17XX_40XX_H_ */