| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
qei_001.h
Go to the documentation of this file.
1 /*
2 * @brief Quadrature Encoder Interface Registers and control functions
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __QEI_001_H_
33 #define __QEI_001_H_
34
35 #include "sys_config.h"
36 #include "cmsis.h"
37
38 #ifdef __cplusplus
39 extern "C" {
40 #endif
41
51 typedef struct {
52 __O uint32_t CON;
53 __I uint32_t STAT;
54 __IO uint32_t CONF;
55 __I uint32_t POS;
56 __IO uint32_t MAXPOS;
57 __IO uint32_t CMPOS0;
58 __IO uint32_t CMPOS1;
59 __IO uint32_t CMPOS2;
60 __I uint32_t INXCNT;
61 __IO uint32_t INXCMP0;
62 __IO uint32_t LOAD;
63 __I uint32_t TIME;
64 __I uint32_t VEL;
65 __I uint32_t CAP;
66 __IO uint32_t VELCOMP;
67 __IO uint32_t FILTERPHA;
68 __IO uint32_t FILTERPHB;
69 __IO uint32_t FILTERINX;
70 __IO uint32_t WINDOW;
71 __IO uint32_t INXCMP1;
72 __IO uint32_t INXCMP2;
73 __I uint32_t RESERVED0[993];
74 __O uint32_t IEC;
75 __O uint32_t IES;
76 __I uint32_t INTSTAT;
77 __I uint32_t IE;
78 __O uint32_t CLR;
79 __O uint32_t SET;
80 } IP_QEI_001_T;
81
86 #ifdef __cplusplus
87 }
88 #endif
89
90 #endif /* __QEI_001_H_ */