| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_ENET_002_RXFILTER_T Struct Reference
IP: Ethernet register block and driver (002)

## Detailed Description

Ethernet Receive Filter register block structure.

Definition at line 102 of file enet_002.h.

`#include "enet_002.h"`

## Data Fields
__IO uint32_t | CONTROL
__I uint32_t | WOLSTATUS
__O uint32_t | WOLCLEAR
uint32_t | RESERVED
__IO uint32_t | HashFilterL
__IO uint32_t | HashFilterH

## Field Documentation

__IO uint32_t CONTROL

Receive filter control register

Definition at line 103 of file enet_002.h.

__IO uint32_t HashFilterH

Hash filter table MSBs register

Definition at line 108 of file enet_002.h.

__IO uint32_t HashFilterL

Hash filter table LSBs register

Definition at line 107 of file enet_002.h.

uint32_t RESERVED

Definition at line 106 of file enet_002.h.

__O uint32_t WOLCLEAR

Receive filter WoL clear register

Definition at line 105 of file enet_002.h.

__I uint32_t WOLSTATUS

Receive filter WoL status register

Definition at line 104 of file enet_002.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/enet_002.h