| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros
BOARD: K9F1G NAND Flash drivers
BOARD: Board specific NAND Flash drivers

## Detailed Description

## Data Structures
struct | K9F1G_ID_T

## Macros
#define | KF91G_NANDFLASH
#define | K9F1G_PAGE_SIZE (2 << 10) /* 2K bytes */
#define | K9F1G_SPARE_START_ADDR ( K9F1G_PAGE_SIZE) /* Spare start address */
#define | K9F1G_SPARE_SIZE (64)
#define | K9F1G_PAGES_PER_BLOCK (64)
#define | K9F1G_BLOCK_COUNT (1024)
#define | K9F1G_READ_1 0x00
#define | K9F1G_READ_2 0x30
#define | K9F1G_READ_ID 0x90
#define | K9F1G_RESET 0xFF
#define | K9F1G_PAGE_PROGRAM_1 0x80
#define | K9F1G_PAGE_PROGRAM_2 0x10
#define | K9F1G_BLOCK_ERASE_1 0x60
#define | K9F1G_BLOCK_ERASE_2 0xD0
#define | K9F1G_READ_STATUS 0x70
#define | NANDFLASH_STATUS_PAGE_PROG_FAIL (1 << 0)
#define | NANDFLASH_STATUS_BLOCK_ERASE_FAIL (1 << 0)
#define | NANDFLASH_STATUS_DEV_READY (1 << 6)
#define | NANDFLASH_STATUS_READ_WRITE_NPROTECTED (1 << 7)
#define | NANDFLASH_PROG_TIME (700 * 1000)
#define | NANDFLASH_BLOCK_ERASE_TIME (3 * 1000 * 1000)
#define | NANDFLASH_READ_TIME (25 * 1000)

## Macro Definition Documentation

#define K9F1G_BLOCK_COUNT (1024)

Definition at line 57 of file lpc_nandflash_k9f1g.h.

#define K9F1G_BLOCK_ERASE_1 0x60

Definition at line 68 of file lpc_nandflash_k9f1g.h.

#define K9F1G_BLOCK_ERASE_2 0xD0

Definition at line 69 of file lpc_nandflash_k9f1g.h.

#define K9F1G_PAGE_PROGRAM_1 0x80

Definition at line 66 of file lpc_nandflash_k9f1g.h.

#define K9F1G_PAGE_PROGRAM_2 0x10

Definition at line 67 of file lpc_nandflash_k9f1g.h.

#define K9F1G_PAGE_SIZE (2 << 10) /* 2K bytes */

Definition at line 49 of file lpc_nandflash_k9f1g.h.

#define K9F1G_PAGES_PER_BLOCK (64)

Definition at line 55 of file lpc_nandflash_k9f1g.h.

#define K9F1G_READ_1 0x00

Definition at line 62 of file lpc_nandflash_k9f1g.h.

#define K9F1G_READ_2 0x30

Definition at line 63 of file lpc_nandflash_k9f1g.h.

#define K9F1G_READ_ID 0x90

Definition at line 64 of file lpc_nandflash_k9f1g.h.

#define K9F1G_READ_STATUS 0x70

Definition at line 70 of file lpc_nandflash_k9f1g.h.

#define K9F1G_RESET 0xFF

Definition at line 65 of file lpc_nandflash_k9f1g.h.

#define K9F1G_SPARE_SIZE (64)

Definition at line 53 of file lpc_nandflash_k9f1g.h.

#define K9F1G_SPARE_START_ADDR ( K9F1G_PAGE_SIZE) /* Spare start address */

Definition at line 51 of file lpc_nandflash_k9f1g.h.

#define KF91G_NANDFLASH

Definition at line 46 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_BLOCK_ERASE_TIME (3 * 1000 * 1000)

tBERS

Definition at line 117 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_PROG_TIME (700 * 1000)

tPROG

Definition at line 115 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_READ_TIME (25 * 1000)

tR

Definition at line 119 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_STATUS_BLOCK_ERASE_FAIL (1 << 0)

Definition at line 107 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_STATUS_DEV_READY (1 << 6)

Definition at line 108 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_STATUS_PAGE_PROG_FAIL (1 << 0)

Definition at line 106 of file lpc_nandflash_k9f1g.h.

#define NANDFLASH_STATUS_READ_WRITE_NPROTECTED (1 << 7)

Definition at line 109 of file lpc_nandflash_k9f1g.h.