| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
usbmsdev.h
Go to the documentation of this file.
1 /*
2 * @brief LPCUSBlib Mass Storage Device Dual core example
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
37 #ifndef __USBMSDEV_H_
38 #define __USBMSDEV_H_
39
40 #define __DATARAM_H_
41
42 /* Includes: */
43 #include "board.h"
44 #include "lpc43xx_dualcore_config.h"
45
46 #include "USB.h"
47 #include <string.h>
48 #include "Descriptors.h"
49 #include "Lib/SCSI.h"
50
51 /* OS Specific includes */
52 #ifdef OS_FREE_RTOS
53 /* FreeRTOS headers */
54 #include "FreeRTOS.h"
55 #include "semphr.h"
56 #include "task.h"
57 #define LOOP_TASKS 1
58 #elif defined(OS_UCOS_III)
59 #include "os.h"
60 #include "cpu.h"
61 #include "os_cfg_app.h"
62 #define LOOP_TASKS 1
63 #else
64 #define LOOP_TASKS 0
65 #endif
66
75 /* Macros: */
77 #define LEDMASK_USB_NOTREADY LEDS_LED1
78
80 #define LEDMASK_USB_ENUMERATING (LEDS_LED2 | LEDS_LED3)
81
83 #define LEDMASK_USB_READY (LEDS_LED2 | LEDS_LED4)
84
86 #define LEDMASK_USB_ERROR (LEDS_LED1 | LEDS_LED3)
87
89 #define LEDMASK_USB_BUSY LEDS_LED2
90
92 #define TOTAL_LUNS 1
93
95 #define LUN_MEDIA_BLOCKS (VIRTUAL_MEMORY_BLOCKS / TOTAL_LUNS)
96
98 #define DISK_READ_ONLY false
99
105 void EVENT_USB_Device_Connect(void);
106
112 void EVENT_USB_Device_Disconnect(void);
113
119 void EVENT_USB_Device_ConfigurationChanged(void);
120
126 void EVENT_USB_Device_ControlRequest(void);
127
136 bool CALLBACK_MS_Device_SCSICommandReceived(USB_ClassInfo_MS_Device_t *const MSInterfaceInfo);
137
142 #endif