| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
HAL_LPC11Uxx.h
Go to the documentation of this file.
1 /*
2 * @brief HAL USB functions for the LPC11Uxx microcontrollers
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __HAL_LPC11UXX_H__
33 #define __HAL_LPC11UXX_H__
34 #include "chip.h"
35 #define __INCLUDE_FROM_USB_DRIVER
36
37 #include "../../USBMode.h"
38
39 #define USBRAM_SECTION RAM2
40
41 #if defined(__CC_ARM)
42 #define __BSS(x) __attribute__ ((section("usbram")))
43 #endif
44 #if defined(__ICCARM__)
45 #define __BSS(x) @ "USB_PACKET_MEMORY"
46 #endif
47
48 /* Terminated Link Mask of USB DMA. */
49 #define LINK_TERMINATE 0x01
50
51 typedef struct {
52 uint16_t BufferAddrOffset;
53
54 __IO uint16_t NBytes : 10;
55 uint16_t Type : 1;
56 uint16_t RateFeedback_Toogle : 1;
57 uint16_t ToogleReset : 1;
58 __IO uint16_t Stall : 1;
59 uint16_t Disabled : 1;
60 __IO uint16_t Active : 1;
61
62 } /* __attribute__ ((packed)) */ USB_CMD_STAT;
63
64 void HAL_Reset (void);
65
66 void HAL_SetDeviceAddress (uint8_t Address);
67
68 #endif // __HAL_LPC11UXX_H__
69