| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
FLASH_COMPARE_MEM_COMMAND_T Struct Reference
IP: Flash/EEPROM programming

## Detailed Description

[Compare memory] command parameter table structure

Definition at line 279 of file flash_001.h.

`#include "flash_001.h"`

## Data Fields
uint32_t | cmd
uint32_t | dst
uint32_t | src
uint32_t | byteNum

## Field Documentation

uint32_t byteNum

Number of bytes to be compared; should be a multiple of 4.

Definition at line 283 of file flash_001.h.

uint32_t cmd

Command code

Definition at line 280 of file flash_001.h.

uint32_t dst

Starting flash or RAM address of data bytes to be compared (a word boundary)

Definition at line 281 of file flash_001.h.

uint32_t src

Starting flash or RAM address of data bytes to be compared (a word boudary).

Definition at line 282 of file flash_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/flash_001.h