| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
LPC_SWM_T Struct Reference
CHIP: LPC8xx Switch Matrix Driver

## Detailed Description

LPC8XX Switch Matrix register block structure.

Definition at line 47 of file swm_8xx.h.

`#include "swm_8xx.h"`

## Data Fields
__IO uint32_t | PINASSIGN [9]
__I uint32_t | RESERVED0 [103]
__IO uint32_t | PINENABLE0

## Field Documentation

__IO uint32_t PINASSIGN[9]

Pin Assign register array

Definition at line 48 of file swm_8xx.h.

__IO uint32_t PINENABLE0

Pin Enable register

Definition at line 50 of file swm_8xx.h.

__I uint32_t RESERVED0[103]

Definition at line 49 of file swm_8xx.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_chip/chip_8xx/swm_8xx.h