| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Memory based file system support
Chan FATFS file system

## Detailed Description

## Functions
void | FATFS_GetBufferInfo (uint8_t **buffer, uint32_t *size)
| Gets Ramdisk Memory information.

## Function Documentation

void FATFS_GetBufferInfo | ( | uint8_t ** | buffer,
|  | uint32_t * | size
| ) |  |

Gets Ramdisk Memory information.

Parameters

  buffer | : pointer to hold the starting address of RAM disk
  size | : Pointer to returned size of the RAM disk

Returns
  None

Note
  This function must be implemented by the application so that the filesystem will be aware of the location of the RAM disk.

Definition at line 362 of file lwip_fs.c.