| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Typedefs
chip_lpc177x_8x.h File Reference
`#include "lpc_types.h"`
`#include "sys_config.h"`
`#include "adc_001.h"`
`#include "can_001.h"`
`#include "dac_001.h"`
`#include "emc_001.h"`
`#include "enet_002.h"`
`#include "gpdma_001.h"`
`#include "gpio_002.h"`
`#include "i2c_001.h"`
`#include "i2s_001.h"`
`#include "lcd_001.h"`
`#include "mcpwm_001.h"`
`#include "qei_001.h"`
`#include "regfile_001.h"`
`#include "rtc_001.h"`
`#include "sdc_001.h"`
`#include "ssp_001.h"`
`#include "timer_001.h"`
`#include "usart_001.h"`
`#include "wwdt_001.h"`
`#include "usb_001.h"`
`#include "eeprom_001.h"`
`#include "crc_001.h"`
`#include "eeprom_17xx_40xx.h"`
`#include "gpio_17xx_40xx.h"`
`#include "uart_17xx_40xx.h"`
`#include "gpdma_17xx_40xx.h"`
`#include "i2c_17xx_40xx.h"`
`#include "i2s_17xx_40xx.h"`
`#include "ssp_17xx_40xx.h"`
`#include "rtc_17xx_40xx.h"`
`#include "emc_17xx_40xx.h"`
`#include "lcd_17xx_40xx.h"`
`#include "adc_17xx_40xx.h"`
`#include "dac_17xx_40xx.h"`
`#include "timer_17xx_40xx.h"`
`#include "iocon_17xx_40xx.h"`
`#include "sysctl_17xx_40xx.h"`
`#include "clock_17xx_40xx.h"`
`#include "fmc_17xx_40xx.h"`
`#include "can_17xx_40xx.h"`
`#include "crc_17xx_40xx.h"`
`#include "enet_17xx_40xx.h"`
`#include "sdc_17xx_40xx.h"`
`#include "sdmmc_17xx_40xx.h"`
`#include "wwdt_17xx_40xx.h"`

Go to the source code of this file.

## Macros
#define | LPC_EEPROM_BASE 0x00200080
#define | LPC_GPDMA_BASE 0x20080000
#define | LPC_ENET_BASE 0x20084000
#define | LPC_LCD_BASE 0x20088000
#define | LPC_USB_BASE 0x2008C000
#define | LPC_CRC_BASE 0x20090000
#define | LPC_SPIFI_BASE 0x20094000
#define | LPC_GPIO0_BASE 0x20098000
#define | LPC_GPIO1_BASE 0x20098020
#define | LPC_GPIO2_BASE 0x20098040
#define | LPC_GPIO3_BASE 0x20098060
#define | LPC_GPIO4_BASE 0x20098080
#define | LPC_GPIO5_BASE 0x200980A0
#define | LPC_EMC_BASE 0x2009C000
#define | LPC_RTC_BASE 0x40024000
#define | LPC_REGFILE_BASE 0x40024044
#define | LPC_WWDT_BASE 0x40000000
#define | LPC_UART0_BASE 0x4000C000
#define | LPC_UART1_BASE 0x40010000
#define | LPC_UART2_BASE 0x40098000
#define | LPC_UART3_BASE 0x4009C000
#define | LPC_UART4_BASE 0x400A4000
#define | LPC_SSP0_BASE 0x40088000
#define | LPC_SSP1_BASE 0x40030000
#define | LPC_SSP2_BASE 0x400AC000
#define | LPC_TIMER0_BASE 0x40004000
#define | LPC_TIMER1_BASE 0x40008000
#define | LPC_TIMER2_BASE 0x40090000
#define | LPC_TIMER3_BASE 0x40094000
#define | LPC_MCPWM_BASE 0x400B8000
#define | LPC_PWM0_BASE 0x40014000
#define | LPC_PWM1_BASE 0x40018000
#define | LPC_I2C0_BASE 0x4001C000
#define | LPC_I2C1_BASE 0x4005C000
#define | LPC_I2C2_BASE 0x400A0000
#define | LPC_I2S_BASE 0x400A8000
#define | LPC_CANAF_RAM_BASE 0x40038000
#define | LPC_CANAF_BASE 0x4003C000
#define | LPC_CANCR_BASE 0x40040000
#define | LPC_CAN1_BASE 0x40044000
#define | LPC_CAN2_BASE 0x40048000
#define | LPC_QEI_BASE 0x400BC000
#define | LPC_DAC_BASE 0x4008C000
#define | LPC_ADC_BASE 0x40034000
#define | LPC_GPIOINT_BASE 0x40028080
#define | LPC_IOCON_BASE 0x4002C000
#define | LPC_SDC_BASE 0x400C0000
#define | LPC_SYSCTL_BASE 0x400FC000
#define | LPC_EEPROM ((IP_EEPROM_001_T *) LPC_EEPROM_BASE)
#define | LPC_GPDMA ((IP_GPDMA_001_T *) LPC_GPDMA_BASE)
#define | LPC_EMC ((IP_EMC_001_T *) LPC_EMC_BASE)
#define | LPC_USB ((IP_USB_001_T *) LPC_USB_BASE)
#define | LPC_LCD ((IP_LCD_001_T *) LPC_LCD_BASE)
#define | LPC_ETHERNET ((IP_ENET_002_T *) LPC_ENET_BASE)
#define | LPC_GPIO ((IP_GPIO_002_T *) LPC_GPIO0_BASE)
#define | LPC_GPIO1 ((IP_GPIO_002_T *) LPC_GPIO1_BASE)
#define | LPC_GPIO2 ((IP_GPIO_002_T *) LPC_GPIO2_BASE)
#define | LPC_GPIO3 ((IP_GPIO_002_T *) LPC_GPIO3_BASE)
#define | LPC_GPIO4 ((IP_GPIO_002_T *) LPC_GPIO4_BASE)
#define | LPC_GPIO5 ((IP_GPIO_002_T *) LPC_GPIO5_BASE)
#define | LPC_RTC ((IP_RTC_001_T *) LPC_RTC_BASE)
#define | LPC_REGFILE ((IP_REGFILE_001_T *) LPC_REGFILE_BASE)
#define | LPC_WWDT ((IP_WWDT_001_T *) LPC_WWDT_BASE)
#define | LPC_UART0 ((IP_USART_001_T *) LPC_UART0_BASE)
#define | LPC_UART1 ((IP_USART_001_T *) LPC_UART1_BASE)
#define | LPC_UART2 ((IP_USART_001_T *) LPC_UART2_BASE)
#define | LPC_UART3 ((IP_USART_001_T *) LPC_UART3_BASE)
#define | LPC_UART4 ((IP_USART_001_T *) LPC_UART4_BASE)
#define | LPC_SSP0 ((IP_SSP_001_T *) LPC_SSP0_BASE)
#define | LPC_SSP1 ((IP_SSP_001_T *) LPC_SSP1_BASE)
#define | LPC_SSP2 ((IP_SSP_001_T *) LPC_SSP2_BASE)
#define | LPC_TIMER0 ((IP_TIMER_001_T *) LPC_TIMER0_BASE)
#define | LPC_TIMER1 ((IP_TIMER_001_T *) LPC_TIMER1_BASE)
#define | LPC_TIMER2 ((IP_TIMER_001_T *) LPC_TIMER2_BASE)
#define | LPC_TIMER3 ((IP_TIMER_001_T *) LPC_TIMER3_BASE)
#define | LPC_MCPWM ((IP_MCPWM_001_T *) LPC_MCPWM_BASE)
#define | LPC_I2C0 ((IP_I2C_001_T *) LPC_I2C0_BASE)
#define | LPC_I2C1 ((IP_I2C_001_T *) LPC_I2C1_BASE)
#define | LPC_I2C2 ((IP_I2C_001_T *) LPC_I2C2_BASE)
#define | LPC_I2S ((IP_I2S_001_T *) LPC_I2S_BASE)
#define | LPC_QEI ((IP_QEI_001_T *) LPC_QEI_BASE)
#define | LPC_DAC ((IP_DAC_001_T *) LPC_DAC_BASE)
#define | LPC_ADC ((IP_ADC_001_T *) LPC_ADC_BASE)
#define | LPC_IOCON ((LPC_IOCON_T *) LPC_IOCON_BASE)
#define | LPC_SDC ((IP_SDC_001_T *) LPC_SDC_BASE)
#define | LPC_SYSCTL ((LPC_SYSCTL_T *) LPC_SYSCTL_BASE)
#define | LPC_CANAF_RAM ((LPC_CANAF_RAM_T *) LPC_CANAF_RAM_BASE)
#define | LPC_CANAF ((LPC_CANAF_T *) LPC_CANAF_BASE)
#define | LPC_CANCR ((LPC_CANCR_T *) LPC_CANCR_BASE)
#define | LPC_CAN1 ((LPC_CAN_T *) LPC_CAN1_BASE)
#define | LPC_CAN2 ((LPC_CAN_T *) LPC_CAN2_BASE)
#define | LPC_CRC ((LPC_CRC_T *) LPC_CRC_BASE)

## Typedefs
typedef IP_EEPROM_001_T | LPC_EEPROM_T
typedef IP_GPDMA_001_T | LPC_GPDMA_T
typedef IP_SDC_001_T | LPC_SDC_T
typedef IP_EMC_001_T | LPC_EMC_T
typedef IP_USB_001_T | LPC_USB_T
typedef IP_ENET_002_T | LPC_ENET_T
typedef IP_REGFILE_001_T | LPC_REGFILE_T
typedef IP_RTC_001_T | LPC_RTC_T
typedef IP_WWDT_001_T | LPC_WWDT_T
typedef IP_USART_001_T | LPC_USART_T
typedef IP_SSP_001_T | LPC_SSP_T
typedef IP_TIMER_001_T | LPC_TIMER_T
typedef IP_MCPWM_001_T | LPC_MCPWM_T
typedef IP_I2C_001_T | LPC_I2C_T
typedef IP_I2S_001_T | LPC_I2S_T
typedef IP_QEI_001_T | LPC_QEI_T
typedef IP_DAC_001_T | LPC_DAC_T
typedef IP_ADC_001_T | LPC_ADC_T
typedef IP_GPIO_002_T | LPC_GPIO_T
typedef IP_LCD_001_T | LPC_LCD_T
typedef IP_CAN_001_AF_RAM_T | LPC_CANAF_RAM_T
typedef IP_CAN_001_AF_T | LPC_CANAF_T
typedef IP_CAN_001_CR_T | LPC_CANCR_T
typedef IP_CAN_001_T | LPC_CAN_T
typedef IP_CRC_001_T | LPC_CRC_T