| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
UsbRom.h File Reference
`#include "DataRam.h"`

Go to the source code of this file.

## Functions
uint32_t | CALLBACK_UsbdRom_Register_DeviceDescriptor (void)
| Call back function registers device descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_ConfigurationDescriptor (void)
| Call back function registers device configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_StringDescriptor (void)
| Call back function registers string descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_DeviceQualifierDescriptor (void)
| Call back function registers device qualifier descriptor array's address to ROM stack.
uint8_t | CALLBACK_UsbdRom_Register_ConfigureEndpoint (void)
| Call back function registers endpoint configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdMsc_Register_InquiryData (void)
| Call back function registers inquiry data.
uint32_t | CALLBACK_UsbdMsc_Register_BlockCount (void)
| Call back function registers block count.
uint32_t | CALLBACK_UsbdMsc_Register_BlockSize (void)
| Call back function registers block size.
uint32_t | CALLBACK_UsbdMsc_Register_MemorySize (void)
| Call back function registers memory size.
uint32_t | CALLBACK_UsbdMsc_Register_InterfaceDescriptor (void)
| Call back function registers interface descriptor.
uint32_t | CALLBACK_UsbdMsc_Register_MSCWrite (void)
| Call back function registers Mass Storage Write.
uint32_t | CALLBACK_UsbdMsc_Register_MSCRead (void)
| Call back function registers Mass Storage Read.
uint32_t | CALLBACK_UsbdMsc_Register_MSCVerify (void)
| Call back function registers Mass Storage Verify.
uint32_t | CALLBACK_UsbdMsc_Register_MSCGetWriteBuf (void)
| Call back function registers Mass Storage Get Write Buffer.