| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
board_nxp_xpresso_11u14.h
Go to the documentation of this file.
1 /*
2 * @brief NXP XPRESSO 11U14 board file
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __BOARD_NXP_XPRESSO_11U14_H_
33 #define __BOARD_NXP_XPRESSO_11U14_H_
34
35 #include "chip.h"
36 #include "board_api.h"
37
38 #ifdef __cplusplus
39 extern "C" {
40 #endif
41
58 #define BOARD_NXP_XPRESSO_11U14
59
60 #if defined(DEBUG_ENABLE) && defined(DEBUGOUT)
61 #undef DEBUGOUT
62 /* Normally routed to printf, but uses too much space, so stub it */
63 #define DEBUGOUT(...)
64 #endif
65
69 #define LEDS_LED1 0x01
70 #define LEDS_LED2 0x02
71 #define LEDS_LED3 0x04
72 #define LEDS_LED4 0x08
73 #define LEDS_NO_LEDS 0x00
74
78 #define BUTTONS_BUTTON1 0x01
79 #define NO_BUTTON_PRESSED 0x00
80
84 #define JOY_UP 0x01
85 #define JOY_DOWN 0x02
86 #define JOY_LEFT 0x04
87 #define JOY_RIGHT 0x08
88 #define JOY_PRESS 0x10
89
94 void Board_UART_Init(void);
95
100 void Board_SSP_Init(void);
101
106 void Board_ADC_Init(void);
107
112 void Board_Buttons_Init(void);
113
118 uint32_t Buttons_GetStatus(void);
119
124 void Board_Joystick_Init(void);
125
130 uint8_t Joystick_GetStatus(void);
131
137 STATIC INLINE void Board_I2C_Init(I2C_ID_T id)
138 {
139 Chip_SYSCTL_PeriphReset(RESET_I2C0);
140 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 4, IOCON_FUNC1);
141 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 5, IOCON_FUNC1);
142 }
143
153 STATIC INLINE void Board_I2C_EnableFastPlus(I2C_ID_T id)
154 {
155 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 4, IOCON_FUNC1 | IOCON_FASTI2C_EN);
156 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 5, IOCON_FUNC1 | IOCON_FASTI2C_EN);
157 }
158
164 STATIC INLINE void Board_I2C_DisableFastPlus(I2C_ID_T id)
165 {
166 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 4, IOCON_FUNC1);
167 Chip_IOCON_PinMuxSet(LPC_IOCON, 0, 5, IOCON_FUNC1);
168 }
169
174 #ifdef __cplusplus
175 }
176 #endif
177
178 #endif /* __BOARD_NXP_XPRESSO_11U14_H_ */