| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions
ccan_18xx_43xx.h File Reference

Go to the source code of this file.

## Macros
#define | CCAN_SEG1_DEFAULT_VAL 5
#define | CCAN_SEG2_DEFAULT_VAL 4
#define | CCAN_SJW_DEFAULT_VAL 0

## Functions
STATIC INLINE void | Chip_CCAN_IntEnable (LPC_CCAN_T *pCCAN, FunctionalState NewState)
| Enable/Disable CCAN Interrupts.
STATIC INLINE uint32_t | Chip_CCAN_GetIntID (LPC_CCAN_T *pCCAN)
| Get the source ID of an interrupt.
STATIC INLINE uint32_t | Chip_CCAN_GetStatus (LPC_CCAN_T *pCCAN)
| Get the CCAN status register.
STATIC INLINE void | Chip_CCAN_GetMsgObject (LPC_CCAN_T *pCCAN, uint8_t msg_num, message_object *msg_buf)
| Get a message object in message RAM into the message buffer.
void | Chip_CCAN_Init (LPC_CCAN_T *pCCAN)
| Initialize the CCAN peripheral, free all message object in RAM.
void | Chip_CCAN_DeInit (LPC_CCAN_T *pCCAN)
| De-initialize the CCAN peripheral.
void | Chip_CCAN_SetBitRate (LPC_CCAN_T *pCCAN, uint32_t bitRate)
| Select bit rate for CCAN bus.
void | Chip_CCAN_ClearStatus (LPC_CCAN_T *pCCAN, IP_CCAN_STATUS_T status)
| Clear the status of CCAN bus.
void | Chip_CCAN_ClearIntPend (LPC_CCAN_T *pCCAN, uint8_t msg_num, uint8_t TRxMode)
| Clear the pending interrupt.
void | Chip_CCAN_Send (LPC_CCAN_T *pCCAN, uint32_t RemoteEnable, message_object *msg_ptr)
| Send a message.
void | Chip_CCAN_AddReceiveID (LPC_CCAN_T *pCCAN, uint32_t rev_id)
| Register a message ID for receiving.
void | Chip_CCAN_DeleteReceiveID (LPC_CCAN_T *pCCAN, uint32_t rev_id)
| Remove a registered message ID from receiving.

## Macro Definition Documentation

#define CCAN_SEG1_DEFAULT_VAL 5

Definition at line 39 of file ccan_18xx_43xx.h.

#define CCAN_SEG2_DEFAULT_VAL 4

Definition at line 40 of file ccan_18xx_43xx.h.

#define CCAN_SJW_DEFAULT_VAL 0

Definition at line 41 of file ccan_18xx_43xx.h.