| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_ENET_001_TXDESC_T Struct Reference
IP: Ethernet register block and driver

## Detailed Description

Structure of a transmit descriptor (without timestamp)

Definition at line 409 of file enet_001.h.

`#include "enet_001.h"`

## Data Fields
__IO uint32_t | CTRLSTAT
__IO uint32_t | BSIZE
__IO uint32_t | B1ADD
__IO uint32_t | B2ADD

## Field Documentation

__IO uint32_t B1ADD

Buffer 1 address

Definition at line 412 of file enet_001.h.

__IO uint32_t B2ADD

Buffer 2 or next descriptor address

Definition at line 413 of file enet_001.h.

__IO uint32_t BSIZE

Buffer 1/2 byte counts

Definition at line 411 of file enet_001.h.

__IO uint32_t CTRLSTAT

TDES control and status word

Definition at line 410 of file enet_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/enet_001.h