| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
BOARD: LPC812 board build options
NXP LPC812 Xpresso board support functions

## Detailed Description

This board has options that configure its operation at build-time.

For more information on driver options see
LPCOpen platform design approach and goals

## Macros
#define | LPC8XX_USE_XTAL_OSC 1 /* Set 0 if using on-chip IRC instead of external oscillator */

## Macro Definition Documentation

#define CHIP_LPC8XX

Definition at line 38 of file sys_config.h.

#define CRYSTAL_MAIN_FREQ_IN (12000000)

Definition at line 52 of file sys_config.h.

#define DEBUG_UART LPC_USART0

Definition at line 49 of file sys_config.h.

#define EXTCLKIN_FREQ_IN (0)

Definition at line 55 of file sys_config.h.

#define LPC8XX_USE_XTAL_OSC 1 /* Set 0 if using on-chip IRC instead of external oscillator */

Definition at line 62 of file board_nxp_xpresso_812.h.

#define PKG_TSSOP20 (1)

Definition at line 61 of file sys_config.h.