IOD Dry for MCM2010 product

Revision Register 0244
This is derived from YS2000 IOP Dry FPGA (revision 0140).

Fixes in rev 0240

This has a fix for the IRIG and HiPaP input signal interference. The signal names for debouncing these two input signals were mistyped and so the HiPaP was looking for a low going value on the IRIG to trigger. This product does not have a IRIG input. Only modification relative to YS2000 is in file debouncer.v.
Addition to rev 0244
There is a fixed trigger out on FPGA pin M17. The trigger has no delay relative to the ping and a fixed duration of 1ms.
