10-32 UNF - 2B 0.440 0.159 0.596

R1.025 0.00_{0.00} A

A

Notes:

1)Motor shaft protrudes .75 in max into adapter

2)Gearbox shall be provided w/o lubrication

3)Gearbox shall have no rear seal

4)Adapter shall accept .25 in diameter shaft

1.063

1.181

0.217

1.139

1.125

0.500 -0.002_{0.000}

0.438 -0.002_{0.000}

0.197

0.865 -0.002_{0.000}

0.100 -0.002_{0.000}

0.597

0.400 0.00_{0.00}

B

B

C

C See Note 1

32 16

0.1250 -0.0005_{0.0000}

Section B-B

0.312 R0.250

0.020 45° X

0.319

Section A-A

1.220

1.220

4x 0.125 THRU

0.532

1.654

1.654

R1.025 0.00_{0.00}

Section C-C

1001799

PS40 Gea rhea d

Sha ft Modifica tions

D

C

B

A A

B

C

D

Monterey Bay Aquarium Research Institute

SCALE

SIZE

CAD FILE:

DWG. NO. B SHEET 1 OF 2

REV.

DATE

APPROVALS

DRAWN

CHECKED

ENGINEER

UNLESS OTHERWISE SPECIFIED

TOLERANCES ARE:

DO NOT SCALE DRAWING

Applica tion

NEXT ASSY

Description

BILL OF MATERIALS

1 2 3 4 5 6 7 8

8 7 6 5 4 3 2 1

THE INFORMATION CONTAINED IN THIS DRAWING IS THE SOLE PROPERTY OF MBARI ANY

REPRODUCTION IN PART OR WHOLE WITHOUT THE WRITTEN PERMISSION OF MBARI IS PROHIBITED.

REVISIONS

REV. DESCRIPTION DATE APPROVED

1 PLACE DIM

1/16 2 PLACE DIM .02 3 PLACE DIM

.005 ANGLES 1 1. DIMENSIONS ARE IN INCHES

2. DIMENSION LIMITS HELD AFTER PLATING.

3. REMOVE BURRS AND SHARP EDGES .015 MAX.

4. MACHINED FILLET RADII .0150-.030.

5. MACHINED DIAMETERS ON A COMMON

CENTERLINE CONCENTRIC WITHIN .OO5

6. PERPENDICULARITY & PARALLELISM OF

MACHINED SURFACES .002 PER INCH.

MAX .012 INCHES FOR SINGLE SURFACE.

PROJECT NO.

PROJECT

MBARI

7700 Sandholdt RD.

Moss Landing, CA 95039

PH: (831) 775-1700

NAME

NAME 9/27/00

XXX ZZZZZZZZ

1:1 MECH ENG ON TORNADO

INITIAL RELEASE

WEIGHT

9/27/00

Shop / Q.C.

Engineer

Inspector

Shop Forema n

NEXT ASSY

Number

K

K 0.735 1.063

3.600 4.725

D

C

B

A A

B

C

D

Monterey Bay Aquarium Research Institute

SCALE

SIZE

CAD FILE:

DWG. NO. B SHEET 2 OF 2

REV.

PS40 Gea rhea d Mounting Deta ils

DATE

APPROVALS

DRAWN

CHECKED

ENGINEER

UNLESS OTHERWISE SPECIFIED

TOLERANCES ARE:

DO NOT SCALE DRAWING

Applica tion

NEXT ASSY

Description

BILL OF MATERIALS

1 2 3 4 5 6 7 8

8 7 6 5 4 3 2 1

THE INFORMATION CONTAINED IN THIS DRAWING IS THE SOLE PROPERTY OF MBARI ANY

REPRODUCTION IN PART OR WHOLE WITHOUT THE WRITTEN PERMISSION OF MBARI IS PROHIBITED.

REVISIONS

REV. DESCRIPTION DATE APPROVED

1 PLACE DIM

1/16 2 PLACE DIM .02 3 PLACE DIM

.005 ANGLES 1 1. DIMENSIONS ARE IN INCHES

2. DIMENSION LIMITS HELD AFTER PLATING.

3. REMOVE BURRS AND SHARP EDGES .015 MAX.

4. MACHINED FILLET RADII .0150-.030.

5. MACHINED DIAMETERS ON A COMMON

CENTERLINE CONCENTRIC WITHIN .OO5

6. PERPENDICULARITY & PARALLELISM OF

MACHINED SURFACES .002 PER INCH.

MAX .012 INCHES FOR SINGLE SURFACE.

PROJECT NO.

PROJECT

MBARI

7700 Sandholdt RD.

Moss Landing, CA 95039

PH: (831) 775-1700

NAME

NAME 9/27/00

XXX ZZZZZZZZ

1:1 MECH ENG ON TORNADO

INITIAL RELEASE

WEIGHT

9/27/00

1001799DWG

Shop / Q.C.

Engineer

Inspector

Shop Forema n

NEXT ASSY

Number