Buoy Section Bullets –

Underway data return from ALTEX vehicle

Rotating Carousel/launcher Accomodates up to 14 data buoys

Integrated inductive data link to communicate between AUV and data buoy

Ice-melting buoy can penetrate up to 1 meter of ice

Compact, gas-activated mechanism for buoy actuatuation

Lithium-based exothermic chemical reaction provides energy for ice melting

Inflatable Argos/GPS antenna provides buoy position

Batteries sufficient for up to three days of life/>50kbytes data return

