Mapping AUV Project Meeting

16 June 2003

Attending:

Dave Caress, Paul McGill, Mark Sibenac, Rob McEwen,  Andy Hamilton, Hans Thomas, Farley Shane

1. Issues with nose design - Farley

a. Found that batteries were modeled too heavy.

b. Reworked modeling of weights and buoyancy.

c. Currently have 21 lbs buoyancy in nose design.

d. Decision – 

i. Add length to the nose to get modeled buoyancy up to 40 lbs before trimming.

ii. Add larger pressure compensator for batteries.

2. CRP syntactic foam order

a. Changes now make it $74K

b. Order now to get foam fabrication going, still have four weeks to finish drawings.

3. Reson Edgetech quote

a. Hans has contacted  Roy Abbott about details of Edgetech electronics mounting – Reson has made some changes. Hans has some more dialog to pursue before we place order.

4. PDR on tail section  - Hans

a. Need to decide between using separate aluminum housing for Kearfott INS or repackaging INS into 17” glass sphere with MVC.

b. Decision: pursue tail design that includes repackaging INS and MVC into a single glass or titanium sphere

