Mapping AUV Project Meeting

5 April 2004

Attending:

Dave Caress, Farley Shane, Rob McEwen, Hans Thomas, Bill Kirkwood, Paul McGill, Mark Sibenac, Karen Salamy, Rich Henthorn

1. Nose

a. Jbox having some difficulties

i. The DC-DC (28V-12V) converter seems to be undersized, and cannot handle the inrush at turn-on. This can be circumvented for now by inserting 12V power past the converter at startup – this can be done on deck prior to deployment.

ii. One of the x-ports is not working – we won’t have the obstacle avoidance sonar working next week.

iii. We also won’t run the CTD next week because we’ve seen it brown out the converter

iv. A new J-box will be built after next week’s sea trials.

2. Midbody

a. Still ready for at sea testing

3. Tail

a. MVC stack and other electronics mounted in the sphere – one more main bracket  to go in.

b. Need to clean up the molds on the Parasci and Kearfott cables.

c. Need to redo the acoustic modem tranducer whip mold jobs.

d. Still need GPS cable to be spliced and molded

e. Mounts for antenna and strobe will go on today.

f. Rob will rewire and close up Kearfott

g. Software

i. Rich has written the Reson control behavior but not yet tested – Rich and Rob will work on testing this.

ii. Rich and Rob will work on acoustic modem abort switch.

iii. Rob now has driver logging environmental data from fan card.

h. Test plan

i. Rob will work on test plan

4. Batteries

a. Replace fuse on #56 – works now but limited to 50 m

b. Li-Co #132 has software problem – Bluefin is supposed to fix today.

c. CTD vehicle has three working batteries, including #95

d. Need to get another battery from Bluefin (already asked for) – now. Will need three batteries to go to 1000 m in June. Bill will talk again with Frank at Bluefin.

