Mapping AUV Project Meeting

20 April 2004

Attending:

Dave Caress, Farley Shane, Rob McEwen, Hans Thomas, Bill Kirkwood, Paul McGill, Mark Sibenac, Karen Salamy, Rich Henthorn

1. Fit on Zephyr: 

a. Last Friday we assembled the vehicle and moved it onto the Zephyr in order to check the fit in the LRS.

i. The existing DMO vehicle cradle works fine – we will build a second cradle at some point.

ii. The vehicle was too long for the current configuration.

iii. The Zephyr crew found that the LRS could be lengthened 11 inches by swapping an extension section for the current fore section.

iv. The Mapping AUV now fits well in the LRS, and swapping the LRS fore-section will be part of standard mobilization.

2. Goal this week – get it in the tank on Thursday

a. Trim and ballast

b. Run missions

c. Log data

3. Next scheduled opportunity for sea trials – Zephyr on Wednesday/Thursday next week (April 28/29).

4. Nose

a. Done except for trimming/ballasting

5. Midbody

a. Done except for trimming/ballasting

6. Tail

a. Need to close up the Kearfott

b. Secure internal tether connector inside tail.

c. Finish magnet insert to operate reed switch for on-deck battery shutoff.

d. Need to fix one more bad mold job on the hotstart cable

e. Need to check all watertight connections.

f. Need to fill tailcone with oil.

g. Drill hole to allow access to enable switch for the pressure switch tied to the drop weight.

h. Need to hook up all of the RF connections

i. Tighten all penetrators on the sphere.

7. Batteries

a. Bill and Dave are close to done with a memo detailing options for an alternative battery package to be presented to Marcia.

