Mass properties of Mapping PV BlankEnd

Output  coordinate System : -- default --

Density = 0.169 pounds per cubic inch

Mass = 20.590 pounds

Volume = 121.837 cubic inches

Surface area = 526.035 square inches

Center of mass: ( inches )


X = 0.000


Y = 1.784


Z = 0.000

Principal axes of inertia and principal moments of inertia: ( pounds * square inches )

Taken at the center of mass.


 Ix = (1.000, 0.000, 0.000)   
Px = 359.350


 Iy = (0.000, 1.000, 0.000)   
Py = 359.350


 Iz = (0.000, 0.000, 1.000)   
Pz = 568.081

Moments of inertia: ( pounds * square inches )

Taken at the center of mass and aligned with the output coordinate system.


Lxx = 359.350
Lxy = 0.000
Lxz = 0.000


Lyx = 0.000
Lyy = 568.081
Lyz = 0.000


Lzx = 0.000
Lzy = 0.000
Lzz = 359.350

Moments of inertia: ( pounds * square inches )

Taken at the output coordinate system.


Ixx = 424.913
Ixy = 0.000
Ixz = 0.000


Iyx = 0.000
Iyy = 568.081
Iyz = 0.000


Izx = 0.000
Izy = 0.000
Izz = 424.913

