Power / Energy




     Requirements


· Net Power







250 W

· Gross Power







290 W

· Nominal Voltage






24 V DC 

· Endurance







260 Hours 


Mechanical / Environment				Requirements     


     


Weight								224 kg (not including hull or buoyancy foam) 





Volume								0.5334 m (21”) O.D. X  1.5 m (59”) long





Depth Capability						4500 m 





Temperature	


		Arctic operation 					-2°C to 5°C


		Shipboard  						-20°C to 10°C


		Shipping							-40°C to 30°C


		Exercise operation					-2°C to 25°C





Vehicle Orientation					Pitch		Roll		


		Launch							+/- 60°	+/- 90°	


		Operation							+/- 30°	+/- 18°	














Acoustics			Allowable Pump Noise TBD with MIT 


Electrical Isolation from Sea		All Connections











