Summary Log

HUGIN Cruise aboard M/V RIG SUPPORTER

20-25 March 2003


20 March



2000 Depart Port Fourchon onboard the RIG SUPPORTER


21 March



1200 Arrived at the operating area



1500 Deployed HUGIN after battery preparations and pre-dive checks

1600 HUGIN stopped responding to commands and is sitting on the seafloor in 450m’s of water 

1700 Commenced grappling efforts within 100m’s of HUGIN to snag a possible net or cable that may have caught the vehicle.

2300 Ceased grappling efforts, no joy.


22 March



1030 HOS INNOVATOR arrived with ROV



1130 ROV recovery operation commenced



1700 ROV at surface with HUGIN



1730 HUGIN retrieved onboard RIG SUPPORTER



2200 HUGIN repaired, recharged and deployed



2210 HUGIN “timed out” and did not dive, commenced recovery


24 March

0100 HUGIN nose recovery line tangled in aft fins and screw.  AUV placed under tow

0700 HUGIN retrieved onboard

1630 Repairs to stern motors completed, HUGIN deployed

1700-2000 Surveyed a mud volcano

2030 HUGIN retrieved onboard; RIG SUPPORTER

departed operating area


25 March



1000 Arrived at Port Fourchon

