SOON pCO2 
1. Device initialization performed by instrument service
Attempts to set instrument clock 
2. Device metadata returned in SIAM datastream
None
3. Instrument-specific service properties
None
4. Initial service property values for this deployment
powerPolicy=ALWAYS
commPowerPolicy=SAMPLING
powerOnDelaySec=0
nominalCurrentMa=1000
currentLimitMa=2000
sampleSchedule= R */0 */0 */1 */0 * * * * GMT *
maxSampleTries=3
sampleTimeoutMsec=60000
5. Results of acceptance test procedures
6. Known-service bugs/deficiencies
First sampling attempt always fails. 
Service causes excessive number of files on instrument CFLASH

Service does not put instrument device metadata into SIAM datastream

Service.initializeInstrument() does not throw Exception on error







