SeaHorse Profiler Status – 05/09/2005

Problems:

· Firmware Problems/Issues

· Bug in Deployment procedure, easy to avoid.

· Bug causing intermittent lock-up, once after 900 profiles, once after 170 profiles.   Watchdog?

· Firmware limitation currently limits depth of profile, apparently resolved.

· Filenumber limitation of 2048 files, need mechanism to delete files.

· Auxillary sensor problems – Needs review/troubleshooting

· Possible issue with usage of internal batteries on CTD.

MSE deployment:

· Mooring/Telemetry Coupling holding up well in near-shore deployment.

· This mooring deployment at Shepard meander possible, with some risk.

· Profiler power usage will allow 6mos of 200m profiles every 4 hours at MSE site (double with lithium batteries ~$1400).

· SIAM/SSDS Service done.

· Tasks.

· Resolve firmware bugs

· Test SIAM Service on MMC

· Design/Specify deepwater mooring.

· Add solar-power system to buoy (Optional).

· Add Locator to buoy/profiler?

· Resolve CTD internal battery issues with Seabird

