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	Deployment
	

	Deployment Date
	


1. Speciality items for this cruise

a. □ Freewave modem deployed spare and cable configured for MSE mooring.
b. □ Surface deployed MMC fully tested.
c. □ Surface secondary deployed MMC fully tested.
2. Cables.

a. □ MMC backplane Console to DB9 cable.

b. □ MMC Surface bulkhead Console to DB9 cable.

c. □ MMC Surface bulkhead to Freewave/Globalstar lab test cable.

d. □ MMC Surface bulkhead to Freewave/Globalstar spare deployed cable. PN 1001532-001

e. □ MMC Surface bulkhead instrument port to DB9 cable for instrument port checking.

f. □ (2) Freewave modem to power supply and DP9 test cable (for lab testing and shipboard operation).

g. □ E/O ODI receptacle test jumper and breakout box.

h. □ (2) BIN wet-mate console cable.

i. □ BIN power and data extension cable for g & h above.

j. □ Optical jumper cables (at least 20 meters).

k. □ MMC chassis 12V power cable.

3. Hardware

a. □ Freewave modems configured for MSE mooring.

b. □ Freewave high gain antenna and cable.

c. □ Freewave low gain antenna.

d. □ MMC Chassis with current release of SideARM, Medusa, RFIO and at least two DPA cards.

e. □ (2) 12V power supplies for MMC chassis and Freewave.

f. □ 60V power supply for ADCP.

g. □ 400VDC power supply for BIN.

h. □ 400VDC start-up box.

4. Cases

a. □ (1`) “MOOS Connector Service Kit”.

b. □ (1) “MOOS Field Service Toolbox”.

5. Instrument Cables and Spares

a. □ (1) Spare Aquadopp battery pack.

b. □ (1) Spare RDI Sentinel battery pack.

c. □ (9) Spare SBE16+ Alkaline D cell batteries.

d. □ (1) Spare Wetlabs shorting jumper.

e. □ Wetlabs to computer test cable.

f. □ Aquadopp to computer test cable and power supply.

g. □ RDI ADCP test and power supply cable.

h. □ SBE16+ test cable.

6. Documentation
a. □ All hardware documentation from project folder.

b. □ Optical system configuration drawing.

c. □ Software commands binder (Mark C. copy).
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