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1) In case of loss of contact with the mooring the position can be verified using the systems ARGOs transponder:

Telnet to: datadist.argosinc.com

Username: MACBRIDE

Password: MONREQU

At the prompt type HELP for a list of commands.  Type HELP,DIAG for help with the diagnostic command.

Telnet access is $0.24/minute.

To retrieve the data for our PTT's, at the prompt type:

PRV/A,2606,DS,,

Our program number is 2606

Our PTT numbers are

39322 - MTM3

44262 - MTM4/MSE

Example:

>telnet datadist.argosinc.com

******* UNAUTHORIZED ACCESS TO THIS NETWORK IS STRICTLY PROHIBITED

Username: MACBRIDE

Password:

     LOGIN AT 106/1527  LAST ACCESS AT 106/1527 UTC

ARGOS READY

/PRV/A,2606,DS,,

02606 44262   2  4 L 2 2007-04-15 23:59:18  36.203  237.101  0.000

      2007-04-16 00:04:48  6         00          232           00

      006 msgs 002>-120dB  Best:  -118  Freq:  649449.5  IQ : 58

02606 44262   2  4 K 2 2007-04-16 00:35:58  36.201  237.121  0.000

      2007-04-16 00:39:38  7         00          232           00

      007 msgs 004>-120dB  Best:  -118  Freq:  649451.4  IQ : 68

      Lat1: 36.201N  Lon1: 122.879W  Lat2: 39.726N  Lon2: 105.708W

/logout

     LOGOUT AT 106/1528 UTC

Connection to host lost.

