CORRECTIONS 5-7-04 REPORT

On page 5 line 5: 

Change “photographic” to “environmental”

On page 6, first sentence of 2.4 text

Change from “…is the S-Tether concept.” to “…..uses a subsurface buoy and S-tether for the link between subsurface and surface buoy.”

Page 9, change head line of last paragraph

Change from “Polyester Cord Reinforced”..to “Nylon Cord Reinforced”

Page 10, last sentence of first paragraph  of 3.4 Cable Design Options

Change from: “Each design as advantageous and disadvantage as discussed below” to

“Each design has advantages and disadvantageous as discussed below.

Page 10 line 5 of Center Conductor Core:
Change from “..fibers can undergo stretch that is considerably more than that of the 0.5 percent limit” to “fibers undergo stretch considerably more than the 0.5 percent limit of..”

Page 10, line 4 from the bottom of page:
Strike the following text: “and the high stiffness of the resulting cables with regard to preventing the conductors and optical fibers from overstretching”

Page 11, first line of text

Change from “..braided strength member..” to “  braided and spliceable strength member”

Page 11, last sentence under High Tension Bend Relief
Change from:“…attachment point and snubber these boots or a molded chain section..” to

“attachment point snubber hoses or an electro-mechanical chain section…”

Page 13, first line of text

Change from “…than wire rope Issues..” to “   than wire rope.  Issues…”

Page 13, second sentence under 4.1 Cable Designs

Line 3: move “are wrapped” to the end of the sentence on line 4

Page 14, add to last line of first paragraph after ..”signal attenuation”

Add:”and reduces the conductor wrap angle required to achieve conductor “comfort”.”

Page 16, third last line of first paragraph

Instead of “spring buoys”  use “surface buoys”…

Page 16, third last line of second paragraph

Add “and drag forces” after “additional windage”

