Project Report

2/10/00 MOOS meeting

Mark Chaffey

First draft of functional requirements

Geographical coverage of equatorial Pacific north to station “P” at 50N and the eastern Pacific requested.

80% of requested measurement areas could be covered by Monterey Bay and out 1000km and the Juan De Fuca ridge complex

Depths range to 6000 meters

80% coverage range to 4000 meters with many sites

Progress since kick-off meeting

First draft of functional requirements many of which are directly applicable to the mooring design

Ed Mellinger 50% complete on establishing an available power baseline based on Oasis solar energy data.

Ed also investigating commercial wave power systems that are potentially suitable

Mark Griese familiarizing himself with dynamics modeling tools used to predict mooring riser cable performance. Now that first draft of the requirements are out he can start working on the performance of concept designs.

Before next meeting

Release revision of functional requirements that includes action items from first release and break-downs for specific MOOS subsystems and projects such as moorings, AUV’s, risers, etc.

Finalize detailed project plan for the year

Develop project test plan, especially for 2001 test deployment

Develop first cut at a series of concept designs that can be used to:

Compare with experiment configurations that come out of the science working groups

Identify design study areas and assign specific design study tasks to specific team members


Identify design studies that we would like to contract for from external experts

