surface_1446-PowerCan_1322
1. Manually-configured instrument settings not handled by service

Unknown?

2. Device metadata returned in SIAM datastream

Couldn't get moos.devices.serialadc.PowerCan instrument state

3. Instrument-specific service properties

captureParams=ALL

statusMinSamples=10

powerWarningLow=9.0

powerOkLow=10.0

powerStatusChannel=ADC99

dataCountCheck=true

4. Initial service property values for this deployment

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.serialadc.SerialAdc$Attributes

serviceName=Mooring power can s/n 002

parentID=1446

currentLimitMa=500

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=9E1469CB-5306-45E4-AFE8-F6290F8C7330

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1322

sampleTimeoutMsec=5000

commPowerPolicy=SAMPLING

serviceStatus=1

logTimeSync=true

startDelayMsec=10000

5. Results of acceptance test procedures

All passed

6. Known-service bugs/deficiencies

Not running against latest firmware version

Power failure detection not configured/tested

Could not get device state metadata?







